        #
        | README file for
        |
        | Windows NT CAPI-Driver for ELSA QuickStep 1000
        | Version 2.10
        |
        | Copyright (c) 1993-97 ELSA GmbH, Aachen (Germany)
        |
        |                                     Subsidiary:
        | ELSA GmbH                           ELSA Inc.
        | Sonnenweg 11                        2150 Trade Zone Blvd.
        | D-52070 Aachen                      Suite 101
        | Germany                             San Jose, CA 95131
        |                                     USA
        |
        | Phone      : +49-241-9177-0         Phone: +1-408-935-0350
        | Support Fax: +49-241-9177-113       Phone:  1-800-272-ELSA
        | BBS (modem): +49-241-9177-981       Fax  : +1-408-935-0370
        | BBS (ISDN) : +49-241-9177-7800      BBS  : +1-408-935-0380
        | CompuServe : GO ELSA                CIS  : GO ELSA
        | WWW        : http://www.elsa.de     WWW  : http://www.elsa.com
        |
        | 02/01/97

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

        Table of Contents

        1.      Overview
        2.      Contents
        3.      Installation
        4.      Notes

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

1.      Overview:

        This file contains notes and changes to the MicroLink
        ISDN drivers.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

2.      Contents:

        This directory contains the following files:

        README.TXT   This file
        LIESMICH.TXT German version of this README.TXT

        SETUP.EXE    Installation Program

        CAPI2032.DLL CAPI Dynamic Link Library for Windows NT

2.1     Driver for CAPI 2.0 and 1TR6 (national ISDN):

        ISDNCAPX.SYS  CAPI version 2.0 driver for ELSA QuickStep 1000
        D channel protocol : 1TR6 (national ISDN)
        B channel protocols: HDLC transparent, bit transparent,
                             X.75, T.70NL, V.120
                             ISO 8208 (X.25), T.90

               - - - - - - - - - - - - - - - - - - - - - - - -

2.2     Driver for CAPI 2.0 and DSS1 (EURO-ISDN):

        DSS1CAPX.SYS  CAPI version 2.0 driver for ELSA QuickStep 1000
        D channel protocol : DSS1 (EURO-ISDN)
        B channel protocols: HDLC transparent, bit transparent,
                             X.75, T.70NL, V.120
                             ISO 8208 (X.25), T.90

               - - - - - - - - - - - - - - - - - - - - - - - -

3.      Installation:

        The following illustration shows the mounting bracket of
        your ISDN plug and play adapter board :
                       _____
                       \    |
                        |   |
                        |   |
                        |   |
                        |   |
                        |___|
                        |___|<- ISDN line connector
                        |   |
                        | o |<- ISDN connection status display (yellow LED)
                        | o |<- ISDN interface status display (green LED)
                        |___|
                                          _
                                         |
                                         |
                                         |
                                         |
         ________________________________|
        |                               _|
        |                              |_ <- ISDN line connector
        |                                |
        |                                o<- yellow LED
        |    _                      __   o<- green LED
        |___| |____________________|  |__|


        The ISDN plug and play adapter board is full software-
        configurable and has NO jumper.

               - - - - - - - - - - - - - - - - - - - - - - - -

        Perform the following steps:

        a) Log on as administrator on your NT - System.

        b) Start the Installation Program SETUP.EXE and perform
           all steps described there.

        c) Shutdown and restart your system.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

4.      Notes:

        The latest information you will always find in the 
        Support BBS ELSA ONLINE or on our homepage http:\\www.elsa.de.

               - - - - - - - - - - - - - - - - - - - - - - - -

        Have fun with your ELSA ISDN board.
