        #
        | README file for
        |
        | ELSA QuickStep 1000
        | Version 2.10
        |
        | Copyright (c) 1993-97 ELSA GmbH, Aachen (Germany)
        |
        |                                     Subsidiary:
        | ELSA GmbH                           ELSA Inc.
        | Sonnenweg 11                        2150 Trade Zone Blvd.
        | D-52070 Aachen                      Suite 101
        | Germany                             San Jose, CA 95131
        |                                     USA
        |
        | Phone      : +49-241-9177-0         Phone: +1-408-935-0350
        | Support Fax: +49-241-9177-113       Phone:  1-800-272-ELSA
        | BBS (modem): +49-241-9177-981       Fax  : +1-408-935-0370
        | BBS (ISDN) : +49-241-9177-7800      BBS  : +1-408-935-0380
        | CompuServe : GO ELSA                CIS  : GO ELSA
        | WWW        : http://www.elsa.de     WWW  : http://www.elsa.com
        |
        | 02/01/97

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

        Table of Contents

        1.      Overview
        2.      Contents
        3.      Installation
        4.      Notes

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

1.      Overview:

        This file contains notes and changes to the
        ISDN drivers.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

2.      Contents:

        This directory contains the following files:

        README.TXT   This file
        LIESMICH.TXT German version of this README.TXT

        CAPI.DLL     CAPI Dynamic Link Library for OS/2

2.1     Driver for CAPI 1.1 and 1TR6 (national ISDN):

        ISDNCAPX.EXE  CAPI version 1.1 driver for ELSA QuickStep 1000
        D channel protocol : 1TR6 (national ISDN)
        B channel protocols: HDLC transparent, bit transparent,
                             X.75, T.70NL, V.120

               - - - - - - - - - - - - - - - - - - - - - - - -

2.2     Driver for CAPI 1.1 and DSS1 (EURO-ISDN):

        DSS1CAPX.EXE  CAPI version 1.1 driver for ELSA QuickStep 1000
        D channel protocol : DSS1 (EURO-ISDN)
        B channel protocols: HDLC transparent, bit transparent,
                             X.75, T.70NL, V.120

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

3.      Installation:

        The following illustration shows the mounting bracket of
        your ISDN plug and play adapter board :
                       _____
                       \    |
                        |   |
                        |   |
                        |   |
                        |   |
                        |___|
                        |___|<- ISDN line connector
                        |   |
                        | o |<- ISDN connection status display (yellow LED)
                        | o |<- ISDN interface status display (green LED)
                        |___|
                                          _
                                         |
                                         |
                                         |
                                         |
         ________________________________|
        |                               _|
        |                              |_ <- ISDN line connector
        |                                |
        |                                o<- yellow LED
        |    _                      __   o<- green LED
        |___| |____________________|  |__|


        The ISDN plug and play adapter board is full software-
        configurable and has NO jumper.

               - - - - - - - - - - - - - - - - - - - - - - - -

        a.) Installation with plug and play:

            If you system supports plug and play you just have to
            install the driver without any parameters.

               - - - - - - - - - - - - - - - - - - - - - - - -

        b.) Installation without plug and play:

            If your system don't supports plug and play, and you
            install the driver without any parameters, the driver
            uses the following defaults:

            I/O-address : 0x160h
            IRQ         : 15

            If this parameters are used by an other programm, you
            have to install the driver with the following
            parameters:

            <Drivername> [/aI/O-address] [/rIRQ]

            e.g.: ISDNCAPI /a160 /r12

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

4.      Notes:

        V.120 under CAPI 1.1 and CFOS (version newer than 07/15/96):

        Enter the following AT-command:

            AT B12 S17=1 S76=1

        Now, the ISDN adapter board tries to get a V.120 connection
        erverytime you dial "ATDn" (n = number)..

        If you want to get back to X.75 mode, you have to enter:

            AT&F

               - - - - - - - - - - - - - - - - - - - - - - - -

        The latest information you will always find in the 
        Support BBS ELSA ONLINE or on our homepage http:\\www.elsa.de.

        Have fun with your ISDN board.
