        #
        | README file for
        |
        | ELSA ISDNmonitor
        |
        | Copyright (c) 1993-97 ELSA GmbH, Aachen (Germany)
        |
        |                                     Subsidiary:
        | ELSA GmbH                           ELSA Inc.
        | Sonnenweg 11                        2150 Trade Zone Blvd.
        | D-52070 Aachen                      Suite 101
        | Germany                             San Jose, CA 95131
        |                                     USA
        |
        | Phone      : +49-241-9177-0         Phone: +1-408-935-0350
        | Support Fax: +49-241-9177-113       Phone:  1-800-272-ELSA
        | BBS (modem): +49-241-9177-981       Fax  : +1-408-935-0370
        | BBS (ISDN) : +49-241-9177-7800      BBS  : +1-408-935-0380
        | CompuServe : GO ELSA                CIS  : GO ELSA
        | WWW        : http://www.elsa.de     WWW  : http://www.elsa.com
        |
        | 02/01/97

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

        Inhaltsuebersicht

        1.      Uebersicht
        2.      Inhalt
        3.      Installation
        4.      Benutzung
        5.      Bemerkungen

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

1.      Overview

        This file contains notes and changes to the ELSA ISDNmonitor
        for OS/2.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

2.      Contents:

        README.TXT             This file
        LIESMICH.TXT           German version of this file

        ISDNMON.EXE            ELSA ISDNmonitor for OS/2

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

3.      Installation:

        Copy the file ISDNMON.EXE to the desired destination path
        and start it from there, for example by a program object
        on your desktop.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

4.      Usage:

        The ELSA ISDNmonitor for OS/2 is a 32-Bit Presentation Manager
        application. The main window shows the following information:

          - B-Channels (B1 and B2)

              Con (Yellow LED):
                Off     = B-Channel not active
                Partial = B-Channel requested
                On      = B-Channel active (charged!)

              Tx (Red LED):
                Off     = No Data sent
                On      = Data sent

              Rx (Red LED):
                Off     = No Data received
                On      = Data received

         - S0 Interface

              S0 Power (Green LED):
                Off     = No S0 Power
                On      = S0 Power

              S0 Activation (Green LED):
                Off     = S0 Bus active
                On      = S0 Bus inactive

              TEI (Green LED):
                Off     = No TEI
                On      = Got TEI

              L2 (Green LED):
                Off     = D-Channel not active
                On      = D-Channel active

        In the system menu you will find two additional entries called
        "About" and "Information". With "Information" you will get further
        information about your CAPI, your driver, your hardware and
        your ISDNmonitor.

        A double-click on the main window will hide the title bar. The
        window position of the ISDNmonitor is saved in its own
        .INI file.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

5.      Notes:

        The ELSA ISDNmonitor for OS/2
        runs only with the ELSA CAPI 1.1 
        Driver Ver. 1.70 or higher.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -
