        #
        | README file for
        |
       	| ELSA PhotoJet, Version 2.1, for Windows 3.11,
	| Windows 95 und Windows NT 3.51
        |
        | Copyright (c) 1994-96 ELSA GmbH, Aachen (Germany)
        |
	|				      Subsidary:
	| ELSA GmbH                           ELSA Inc.
	| Sonnenweg 11                        2150 Trade Zone Blvd.
	| D-52070 Aachen                      Suite 101
	| Germany                             San Jose, CA 95131
	|                                     USA
	|
	| Phone      : +49-241-9177-0         Phone: +1-408-935-0350
	| Support Fax: +49-241-9177-213       Phone:  1-800-272-ELSA
	| BBS (modem): +49-241-9177-981       Fax  : +1-408-935-0370
	| BBS (ISDN) : +49-241-9177-7800      BBS  : +1-408-935-0380
	| CompuServe : GO ELSA                CIS  : GO ELSA
	| WWW        : http://www.elsa.de     WWW  : http://www.elsa.com
	|
        | 31.07.96, rz


        Table of Contents

        1.      Overview
        2.      Contents
        3.      Installation
        4.	History
	5.      Release notes
	6. 	Known Bugs and operating notes

--------------------------------------------------------------------


1.      Overview

        This disk contains the Plug In software for the
	ELSA PhotoJet adapter for Windows NT 3.51 resp. 4.0
	running on a DEC-Alpha-Workstation.


--------------------------------------------------------------------

2.      Contents

AIO_au~1.8b_	Selection filter
Aio_ma~1.8b_ 	Matrix filter
Amcc16.dl_	Setup DLL
Date.doc	internal file
Elsa_d.wri	Answerfax in German
Elsa_e.wri	Answerfax in English
mscomstf.dll	Setup DLL
mscuistf.dll	Setup DLL
msdetstf.dll	Setup DLL
msinsstf.dll	Setup DLL
msshlstf.dll	Setup DLL
msuilstf.dll	Setup DLL
Photojet.bi_ 	Binary file for the DSP
Photojet.ex_ 	Server for Windows 3.11
Photojet.fo_ 	System font for PhotoJet
Photojet.inf 	Installation script for Windows 95
Photojet.po_ 	Internal help file
Photojet.sy_ 	Windows NT driver
Photomat.po_ 	Internal help file for the selection tool
Ruler.dl_ 	Dialog element
setup.exe	Setup programm
setup.inf	Information file for the setup program
Taster.dl_ 	Dialog element
Uninst.ex_ 	Uninstaller
Vphoto.vxd 	Windows 95 driver
Vphotod.38_ 	Windows 3.11 driver
LIESMICH.TXT   	This file in German
README.TXT	This file 


---------------------------------------------------------------------

3.      Installation

	The Installation program SETUP.EXE runs under
	WindowsNT 3.5 resp. 4.0 for DEC-Alpha-Workstations.
	
	
	After starting the computer, insert the installation disk with
	the PhotoJet software into drive a:.	

3.1	Windows NT 3.51 resp. 4.0:
	Start Windows NT 3.51 resp. 4.0, open the Filemanager and change to
	drive a:. Choose the SETUP.EXE file and start it.
	After choosing the language the installation routine will
	run automatically.


----------------------------------------------------------------

4.      History

	This section describes changes to the previous releases
	of this	disk.
	
4.1	What is new in version 1.10, 27. March 1996

	- The CombiJet functions are added to the dialog surface.

	- The user data file is set up to the Version 1.2
	  (older user data files are no longer valid and must
	  be deleted)

	- Position of the dialogbox will be stored.

	- Gaussian, b/W edges and b/W gradient filters don't work
	  with CombiJet. If one of these filters is active, then all
	  the other CombiJet filters will be disabled.


4.2	What is new in version 1.11, 28. March 1996

	- New cursor shape in source image.


4.3	What is new in version 1.12, 25. April 1996

	- Two and more PhotJet adaptors can be used for improved
	speed-up in calculation (80% to 90% faster). Gaussian filter
	archives no speed-up.


4.4	What is new in version 1.13, 28. May 1996

	- Gaussian filter adjustable in the range of 0.1 to 20.

	- New cursor shape for overview image.

	- New installation programm with uninstall option.


4.5	What is new in version 2.1, 28. June 1996

	- The AIO selection tool was added to the software.

	- The answer fax was added to the installation routine.


4.6     What is new in version 2.11, 9. August 1996

	- All known bugs of version 2.1 are removed.
	
---------------------------------------------------------------------

5.	Software notes        

5.1	Clustering of PhotoJet boards.

	It's possible to cluster up to three PhotoJet boards in a
	system at the same time. The PhotoJet server will recognize
	the number of the installed Photojet boards automatically
	and the Plug In software will organize them.


---------------------------------------------------------------------

6.	Known bugs and operating hints        

6.1	During the installation of the PhotoJet software the 
	error message
	
	"The Photoshop 3.0x is not installed or the file
	"photos30.ini" is not present." 	
	
	appears.
	
	Please make sure that the Adobe Photoshop is installed
	correctly and that the file PHOTOS30.INI was copied into
	the directory "C:\Windows\". If it isn't present, please
	copy the file into this	directory and start the installation
	of the PhotoJet software again. 

6.2	Please close the PhotJet server before you try to uninstall
	the Plug-In software. 
