	#
	| README file for
	|
	| ELSA WINNER AutoCAD/DOS driver, ver 4.22.16
	|
	|	GLoria
	|	WINNER 1000 (ISA/EISA, VL, PCI)
	|	WINNER 1000AVI
	|	WINNER 1000ISA
	|	WINNER 1000PRO
	|	WINNER 1000PRO/X
	|	WINNER 2000 (ISA/EISA, VL)
	|	WINNER 2000PRO
	|	WINNER 2000PRO/X
	|
	| Copyright (c) 1993-96 ELSA GmbH, Aachen (Germany)
	|
	|                                     Subsidary:
        | ELSA GmbH                           ELSA Inc.
        | Sonnenweg 11                        2150 Trade Zone Blvd.
        | D-52070 Aachen                      Suite 101
        | Germany                             San Jose, CA 95131
        |                                     USA
        |
        | Phone      : +49-241-9177-0         Phone: +1-408-935-0350
        | Support Fax: +49-241-9177-213       Phone:  1-800-272-ELSA
        | BBS (modem): +49-241-9177-981       Fax  : +1-408-935-0370
        | BBS (ISDN) : +49-241-9177-7800      BBS  : +1-408-935-0380
        | CompuServe : GO ELSA                CIS  : GO ELSA
        | WWW        : http://www.elsa.de     WWW  : http://www.elsa.com
        |
        | 05/10/96, fc


	Table of Contents

	1.      Overview
	2.      Directory Contents
	3.      Installation
	4.      Notes
	5.      Release Notes, Caveats and Known Problems


------------------------------------------------------------------------

1.      Overview

	This directory contains the WINNER ELSAicon driver for
	AutoCAD R12, AutoCAD R13, 3D Studio, AutoShade V 2.1
	and other programs with the ADI 4.2 interface.

        AutoCAD R11 is not supported.

------------------------------------------------------------------------

2.      Directory Contents

	The directory ACAD holds the following files:

	README          the file you currently look at
	LIESMICH        German version of README
	ELSAADI.EXE     self-expanding archive file:  The list of
			files produced can be found in ADI2-U.ASC or
			the manual, respectively.

        ELSAMENUE.EXE   self-expanding archive file for ELSAICON.
        ELSADWG.EXE
        ELSATOOL.EXE

------------------------------------------------------------------------

3.      Installation

	The Installation is described in the file ADI2-U.ASC or
	in the manual's chapter "Installation".


------------------------------------------------------------------------

4.      Notes

	The configuration of the driver is described in the file
	ADI2-U.ASC or in the manual's chapter "Installation".

	Special functions of the driver as well as extensions over
	the ADI specification can be found  in the file ADI2-U.ASC
	or in the manual's chapter "Configuration", "Additional
	AutoCAD Commands", and others.


------------------------------------------------------------------------

5.      Release notes, caveats and known problems


        Changes from Version 4.22.15 to 4.22.16
        ---------------------------------------

        Problems Resolved:

        1) Config Menu

        Config parameters which do not force a reinitialistion
        of the driver, like menu colors for example, were not
        saved up in the parameter file.


        Changes from Version 4.22.14 to 4.22.15
        ---------------------------------------

        Problems Resolved:

        1) Polygons

        Narrow polygons were not displayed correctly in all cases.

        2) Trim command

        During TRIM commands parts of the cutting edge were temporarily
        not highlighted.


        Changes from Version 4.22.13 to 4.22.14
        ---------------------------------------

        Problems Resolved:
        ------------------

        1) Concave Polygons

        Concave polygons will be represented correctly now.


        2) AutoCAD Render

        Calling the AutoCAD Render twice caused a heap error.
        This is solved.

        Known Problems
        --------------

        1) Polygons

        When a display list is disabled, clipped, concave polygons
        could be drawn incorrectly in some cases.


        Changes from Version 4.22.12 to 4.22.13
        ---------------------------------------

        Problems Resolved:
        ------------------

        1) 16-bit display list (DL)

        Switching from 32-bit DL to 16-bit DL caused a shutdown of the
        system.

        2) Cursor

         a) 256 colors (8bpp)

            While using the palette INVERSE the cursor was
            drawn incorrectly.

         b) True Color

            - the cursor was drawn incorrectly,

            - there was no cursor visible while editing text fields
              within the config menu.


        3) Erasing and palette INVERSE

        When erasing drawing elements, the corresponding bounding box
        was drawn black.

        4) AutoCAD and GENIUS

        Some edit commands like dimensioning of circles or arcs rsp.
        or moving dimensioned text caused a shutdown of the system.

        5) Timing

        The driver now uses the default display mode set by WINSETUP
        as long as no other display mode is set in the configuration
        menu or the ELSAADI.PRM file.

        6) Fonts

        A bug introduced with version 4.22.10 did not allow to load
        other fonts than the system font. This is fixed.

        Known Problems
        --------------

        1) Trim command

        During TRIM commands parts of the cutting edge is temporarily
        not highlighted.

        2) AutoCAD Render

        Calling the AutoCAD Render twice causes a heap error.

        Workaround: Reconfigure the render display for each render
        action.

        3) ELSArender

        -ELSArender is not supported for AutoCAD Release 13.

        -some rendered objects will be represented incorrectly.

        4) DPMS Power Management

        Key strokes have no effect on the power management.

        5) concave polygone

        The handling of some special concave polygone is incorrect.


        Changes from Version 4.22.11 to 4.22.12
        ---------------------------------------

        Problems Resolved:
        ------------------

        1) Grid:

        When editing with grid turned on, the grid was erased around
        the changed drawing element.

