	#
	| README file for
	|
	| ELSA WINDOWS 3.1X MULTIman Driver, Ver. 1.22
	| for
	|
	|       WINNER 2000PRO (VL/PCI)
	|       WINNER 2000PRO/X
	|
	| in combination with one or more
	|
	|       WINNER 2000PRO (VL/PCI)
	|       WINNER 2000PRO/X
	|
	| or
	|
	|       WINNER 2000PRO|PRO/X (PCI)
	|       WINNER 2000PRO/X
	|
	| in combination with one
	|
	|       WINNER 1000ISA
	|
	|
	| Copyright (c) 1994-96 ELSA GmbH, Aachen (Germany)
	|
        |                                     Subsidary:
        | ELSA GmbH                           ELSA Inc.
        | Sonnenweg 11                        2150 Trade Zone Blvd.
        | D-52070 Aachen                      Suite 101
        | Germany                             San Jose, CA 95131
        |                                     USA
        |
        | Phone      : +49-241-606-0         Phone: +1-408-935-0350
        | Support Fax: +49-241-606-6399      Phone:  1-800-272-ELSA
        | BBS (modem): +49-241-606-9800      Fax  : +1-408-935-0370
        | BBS (ISDN) : +49-241-606-9820      BBS  : +1-408-935-0380
        | CompuServe : GO ELSA               CIS  : GO ELSA
        | WWW        : http://www.elsa.de    WWW  : http://www.elsa.com
        |
        | 02/01/96, qn


	Contents

	1. Overview
	2. Disk Contents
	3. Installation
	4. Switching to "One-screen" Windows
	5. Release Notes
	6. Known Bugs and Operating Notes


------------------------------------------------------------------------

1.      Overview

	This disk contains the drivers and tools for the Windows
	multi-screen dispatcher MULTIman and the ELSA WINNER Windows
	drivers required for this operating mode.

	These drivers allow the Windows desktop to be spread over two
	or more monitors on systems equipped with two or more ELSA
	graphics boards, providing the advantage of a considerably
	larger workspace.

	Please note that only special combinations of ELSA WINNER
	graphic boards are allowed.
	The MULTIman driver supports the following combinations of ELSA
	graphics boards:

	first board:
		WINNER 1000ISA [1|2] MB

	second board:
		WINNER 2000PRO | PRO/X [PCI] [2|4|8] MB

	or

	first board:
		WINNER 2000PRO | PRO/X [VL,PCI] [2,4,8] MB

	all other boards:
		WINNER 2000PRO | PRO/X [VL|PCI] [2|4|8] MB


	Combinations with VL and PCI boards are not supported.
        You can use only boards with the same VIDEO RAM.
        With the WINNER 1000ISA only WINNER 2000PRO|PRO/X-PCI
        boards can be used. The PRO and the PRO/X boards should not
        be used	together, too.

	No additional VGA-graphics boards can be operated in the
	computer.

	Up to four boards are supported. With four boards there is the
	possibilty to choose a quadratic (2x2) monitor placement.

	The board with the smallest memory equipment determines the
	highest vertical or horizontal resolution.


------------------------------------------------------------------------

2.      Disk Contents

	DATE    .DOC    file identifying the disk, prod. date, etc.
	README  .TXT    file you currently read
	LIESMICH.TXT    german version of this file

	MULTIMAN.DRV    MULTIman driver file
	WINIC31. DLL     Driver extension file
	WINNER08.DRV    Windows driver for 256 colors
	WINNER16.DRV    Windows driver for 65535 colors
	WINNER32.DRV    Windows driver for 16 million colors


------------------------------------------------------------------------

3.      Installation

	Requirements:

	It is required that Windows runs on each of the boards (in
	one-screen mode) with the ELSA drivers version 3.31 or newer.
	The ELSA WINNER Windows drivers must already be installed before
	you install MULTIman.

	About 3 Mbytes of disk space must be available on the harddisk
	on which Windows is installed.

	The automatic installation and the following instruction
	assume that your secondary and all following boards are
	WINNER 2000PROs or WINNER 2000PRO/Xs.

	Installation Procedure from WINNERware CD:

	First start Windows in your normal configuration. This should
	be on the first board.

	Start the program "SETUP" from the WIN31 directory of your board.
        (e.g.: WINNER\2000PROX\WIN31\SETUP.EXE)
	First the program will ask you to install newer Windows drivers.
	You can do this. After that the SETUP program opens a new
	dialog box where you can choose to install MULTIman or
	the ELSA Utilities. Please choose the "MULTIman" installation
	now. The program will ask you to insert the ELSA disk
	"MULTIman". Now MULTIman will be installed on your harddisk.
	But it won't be configured.

	MULTIman configuration:

	Terminate the SETUP program and start the WINman utility from
	group "ELSAware". Please choose the resolution of the first
	Windows screen.
	Then you can click the button "Change MULTIman". In the
	following dialog box you can choose the number of your WINNER
	screens. After that please entry the virtual resolution for the
	first screen and the physical and virtual resolution for the
	other screens. At the end you have to entry a refresh rate for
	each screen.

	ATTENTION:      Please pay attention to the specifications of
			your monitors, to avoid damages. You can find
			informations in the documetations of the
			monitors.

	Confirm the dialog box with "OK" and save the graphics mode.
	Please shut down all DOS-applcations, because a restart of
	Windows is necessary now.


------------------------------------------------------------------------

4.      Switching to "One-screen" Windows

	The installation of MULTIman modifies your Windows display
	configuration in the SYSTEM.INI file. To switch back to the
	normal one-screen configuration, proceed as follows:

	Start the WINman utility from the group ELSAware again and
	choose the button "Change MULTIman". There you can switch to
	"One-screen" Windows. Save this grafikmode and after the next
	restart you are able to work with the "One-screen" mode again.


------------------------------------------------------------------------

5.      Release Notes

	This section describes changes made to this disk compared with
	older versions.

	MULTIman ver 1.10:
	- Up to four boards supported.
	- Reverse monitor order for horizontal solutions.

        MULTIman ver 1.20:
        - New init code and windows drivers

        MULTIman ver 1.22
        - Update for POWERdraft for AutoCAD


------------------------------------------------------------------------

6.      Known Bugs and Operating Notes

        none
