miro Computer Products AG                                              22.11.96

miroCRYSTAL 22SD twin                                              Version 1.01

WINDOWS 95 driver

IMPORTANT INSTALLATION INSTRUCTIONS
===============================================================================
Start Windows using the VGA drivers before installing the miro drivers!

Remove all other VGA boards from your computer or, if there is an onboard 
VGA on the mainboard, disable the onboard VGA.

The current Windows 95 drivers (Rev 1.00) do not support single screen configu-
ration on the base card. Please boot the piggy board (lower VGA connector and 
standard settings: both Dip switches off) in case you want to run Windows 95 in 
single screen configuration.

The Windows 95 driver software is configured for installation from CD-ROM. 
In case your copy is available on disk only (beta status, update, etc.), copy 
the content of the Windows 95 driver disks to any directory on your hard disk 
first:
E.g. to copy from A: to directory C:\TMP: "XCOPY A:\*.* C:\TMP /S"
The installation can be done Windows 95 compliant afterwards. (Refer to 
Installation Guide.)

Installation of miro Windows 95 drivers and miroWINTOOLS
========================================================
* If you have not done so already, start your computer
* Click the Start menu
* Click on the RUN... Icon
* Enter the command "X":\SETUP
* The miro*win install window opens
* Select your desired language and click "Install"
* The miro Windows 95 drivers and miroWINTOOLS will be copied to your system
* The Settings folder appears.

Using Twinface configuration:
During the first installation you have to restart your sytem after you have 
chosen "miro S3 Twin PCI" for the graphicboard and "miro Twinface" for your 
Monitor. After the restart you can select the monitors in the new tab "Twinface" 
in the "Display Properties". Board "0" stands for the main graphic board (upper
connector), Board "1" stands for the piggy board (lower connector). You have to
restart the system again after you have chosen the monitors. After the restart 
you can change resolution and colour depth. For changing resolution and color 
depth please use the tab "Twinface" in the "Display Properties" dialog box, 
since the Windows 95 standard method (the tab "Settings") whould not offer 
every available combination of resolutions.

LIMITATIONS
===============================================================================
miroSCREENADJUST              Do not use with fixed-frequency monitors.
                              Do not change the image size and position
                              so that they differ from the default settings 
			      too much, because doing so might damage the 
                              monitor.
                              In Twinface configuration:
                              Please make sure that no output limitations are 
                              chosen in miroPINBOARD (use only left screen/only 
                              right screen), while miroSCREENADJUST is running.

miroTINTCONTROL               In 16/32 bit only the main card is supported.
                              In Twinface configuration both screens are 
                              calibrated simultanously in any color depth. In 
                              case two different monitors are used, only one can 
                              be calibrated optimal.
miroPOWERSAVE                 Works, if choosen as screensaver and selected miro 
                              monitor supports power saving. In case you are not 
                              sure, if one of your monitors supports power
                              saving, you should choose a standard monitor
                              (multi frequency monitor) with an according line
                              frequency. That way you make sure that 
                              miroPOWERSAVE would not try to turn off that 
                              monitor.
                              The internal Windows 95 power saving does not work 
                              in Twinface configuration.
 
===============================================================================

PROBLEM              	      SOLUTION
===============================================================================
You cannot enter anything     Press <ALT>.
in the DOS box

Black screens while AVIs are  Sorry about that. No solution yet.
played on "full screen" in    Will be fixed in next Release.
Twinface configuration.

General:
======
1.) In case Windows 95 doesn't start VLB computers, you can change the base 
    address for the linear memory adressing:

        System.ini:
        [Display]
        LinBase=<Address> (MB)

        i.e. 64, 128, or 192

2.) A DIB engine driver is not usable for Video for Windows, but the
    optimized drivers can be fully used, if the miroPINBOARD will set the 
    entries depending on the selected display mode in the Win.ini file.

    ->If possible, start the miroPINBOARD always starting Windows 95. 
      The miroPINBOARD will correct the entries of Video for Windows 
      automatically. 


3.) Using the miroPINBOARD it may happen that switching from the
    virtual modes to the real modes doesn't work at once. In this case we
    recommend to switch into the real mode resolution (640 x 480) first and
    after this to a higher resolution.


