

Before installing the video drivers, you will need to create a diskette
from the disk image (WDC24T.DSK). To create a diskette, do the following:

-  Insert a high density (1.44MB) floppy diskette into the A: drive

-  Type INSTALL <driveletter:> <enter>

-  Once the diskette is created, read the README.TXT file on the diskette
   for complete installation instructions.


