*******************************************************************************
************************* Lotus 1-2-3 2.3 Driver ******************************
*******************************************************************************

Installation
------------
1.  Insert the 928Movie DOS Drivers disk in the appropriate disk drive and
    change the current drive/directory path to the one which contains Lotus
    1-2-3.

2.  Copy the following files from the \LOTUS subdirectory on the 928Movie DOS
    Drivers disk to the directory which contains Lotus 1-2-3:

        123txt25.drv
        123txt43.drv
        123d768.drv
        123s768.drv
        123d600.drv
        123s600.drv
        123text.drv (Steve E to check)

4.  Type INSTALL and press Enter to run the Lotus 1-2-3 install program.

5.  Press Enter to continue.

    You will be presented with several menu choices. Follow the directions
    on the screen and perform the following steps:

    a.  Select "Change Selected Equipment".
    b.  Select "Modify the Current Driver Set".
    c.  Select "Text Display".
    e.  Select "Graphics Display".
    f.  Select the desired S3 text display driver. Do not select the drivers
        for dual display. This configuration is not supported by your computer.
    g.  Press Esc to return to the previous menu.
    h.  Select "Save the Current Drive Set".
    i.  Press Enter to continue.
