 Installing GrafixStar 550 for Windows 3.1
              ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

Note: Make sure that Windows is set up for a Standard VGA display before you
install your GrafixStar 550 card.

1.  Switch off your computer.
2.  Remove your old display adapter or disable your system's built-in display 
    controller (refer to the documentation supplied with your system).
3.  Install the GrafixStar 550 card in a spare PCI expansion slot and connect
    your monitor.
4.  Switch your computer back on.
5.  Insert the VideoLogic Software Library CD-ROM into your CD-ROM drive.
6.  Start Windows, click the File menu in Program Manager, and click Run.
7.  Browse to the file \gs550\win31\disk1\install.exe on your CD-ROM drive, 
    and click OK.
8.  Follow the instructions that appear on the screen.
9.  At the end of the installation, Windows will restart. On some systems
    the restart might fail with the following error message "Error loading 
    cirrus.drv". In this case, copy the file c:\windows\system\546x.drv to 
    c:\windows\system\cirrus.drv. Windows will now start.