-----------------------------------------------------------------------------

               H E W L E T T  P A C K A R D  C O M P A N Y

         HP ProLiant Support Pack (PSP) for Novell NetWare Help

                              Version 6.40a

-----------------------------------------------------------------------------
1. What is a ProLiant Support Pack (PSP)
2. Minimum OS Requirements for the PSP
3. NetWare Red-box Installation
4. Contents of PSP v6.40a
   4.1 NetWare PSP
   4.2 New features included in this PSP
   4.3 New and updated drivers/components in this PSP
   4.4 Drivers removed from this PSP
5. Software Installation
   5.1 Command Line Deployment Using CPQDPLOY.NLM
   5.2 Graphical (NUT-based) Deployment using CPQDPLOY.NLM
   5.3 Command-Line by Individual Package
   5.4 Graphical (NUT-based) Deployment by Individual Package
   5.5 List of Command-line parameters
   5.6 Installation Examples
5. Log files
6. FAQ

-----------------------------------------------------------------------------
1. What is a ProLiant Support Paq (PSP)

A ProLiant Support Paq (PSP) is a bundle of software packages.  Each package
contains an individual driver, utility, or agent software which comes
self-contained with all of the necessary support software for that package.
As an example, the  storage driver package containing CPQSCSI.HAM will
have the associated Novell and HP files, such as NWPA.NLM and
CPQSHD.CDM, that were used during HP's rigorous software testing
included in the package.  Each package contains an NLM extraction utility
to unpack the compressed package contents.

CPQDPLOY.NLM is provided as a package manager for installation of multiple
packages, either through command-line or a NUT-based interface.
CPQDPLOY.NLM uses a bundle XML definition file in the format (BP000xxx.XML)
to determine what packages belong in a bundle, which operating systems are
supported, and other relevant information.

Each package is also installable individually through either its own
command-line or NUT-based interface.  Each individual package has a unique
package number assigned to it by HP.  The packages will always have the
format CP0xxxxx.NLM.

*NOTE: The PSP is HP's replacement for the now withdrawn
       CPQNSSU (NSSD) utility.

*NOTE: The ProLiant Support Pack (PSP) is the HP rebranded name for the
       former Compaq Support Paq (CSP)

The purpose of a PSP is to provide customers with the latest software,
utilities, and drivers for HP Proliant servers. 

 
2 Minimum OS Requirements for the PSP

The PSP currently is shipped as a single bundle that provides support
for NetWare v5.1, and NetWare v6.0.  The PSP expects that you have at a
minimum the following requirements:

   NetWare v4.2    Not Supported
   NetWare v5.1    Base installation.  However, Support Pack 5 or later
                   is recommended.
   NetWare v6.0    Base installation.  However, Support Pack 2 or later
                   is recommended.

*NOTE: NetWare v4.2 is no longer supported as of v6.00.  The last version of
       the CSP for NetWare v4.2 is available on the NetWare v4.2 driver page
       on www.compaq.com/support/files

*NOTE: Small Business versions of the above versions of NetWare are also
       supported.

The PSP is intended to be used after OS installation to update drivers
and install HP-specific utilities (such as Power Management, Health,
etc), agents (Foundation, Server, LAN, and Storage), and Compaq Survey.
HP recommends that the PSP be re-installed after any Novell Consolidated
Support Packs have been installed to ensure that all drivers and utilties
are at the latest versions.


3 NetWare Red-box installation

While the PSP cannot be used during initial NetWare red-box installation,
HP does provide the necessary drivers for red-box installation on the
Smart Start CD in the \COMPAQ\DRIVERS\(OS version) subdirectory in flat
file format.

Support for red-box installations can be accomplished by copying the
contents of the above directory off the Smart Start CD into the
C:\NWUPDATE directory on the server after the hard drive has had a DOS
partition defined and formatted, but prior to NetWare's driver detection.

After the installation has completed, use the PSP as described in
Section 5 to 'complete the server'.

                      
4. Contents of PSP v6.40a

4.1 NetWare PSP

*Note: These are listed in component number order.  Because of load
       dependencies, this is not the order in which drivers are installed
       by the HP Deployment Utility.

  Files Included  OS Suptd               Description
  ==============  ========   ================================================
   CPQDPLOY.NLM   51/60      HP ProLiant Deployment Utility v6.40a
   BP000163.XML   51/60      Bundle installation XML file for CPQDPLOY.NLM
   CPQCSP.TXT                This file
   CP003440.NLM   51/60      Supports the Compaq NetFlex-3 Ethernet Adapters
                               (CPQNF3.LAN)
   CP003441.NLM   51/60      Supports the Fast Ethernet Adapter from HP 
                               (N100.LAN)
   CP003442.NLM   51/60      Supports the HP Gigabit Adapter/Module (N1000.LAN)
   CP003443.NLM   51/60      Supports the HP NC77xx/NC67xx Gigabit Server 
                               Adapter (Q57.LAN)
   CP003444.NLM   51/60      Provides the HP Virtual Adapter Driver with 
                               Advanced Server Features (QASP.LAN)
   CP003445.NLM   51/60      Supports the SysKonnect FDDI Adapters
                               (SKFPNW.LAN)
   CP003446.NLM   60         Provides the hp ProLiant ACPI Platform Support
                               Module for NetWare v6.x (CPQACPI.PSM)
   CP003447.NLM   51/60      Provides the hp ProLiant MPS Platform Support Module
                               for NetWare 5.x and NetWare 6.x (CPQMPK.PSM)
   CP003448.NLM   51/60      Supports the Compaq Remote Insight Adapter
                               (CPQRI.NLM)
   CP003449.NLM   51/60      Provides the hp ProLiant iLo Management Interface
                               Driver (CPQCI.NLM)
   CP003450.NLM   51         Provides the AMI IDE/ATA/ATAPI UDMA Host Adapter
                               Module (MEGAIDE.HAM)
   CP003451.NLM   60         Provides the NetWare NWPA MegaRIDE HAM Driver
                               for NetWare v6.0 (MEGARIDE.HAM)
   CP003452.NLM   51         Provides the NetWare NWPA MegaRIDE HAM Driver
                               for NetWare v5.1 (MEGARIDE.HAM)
   CP003453.NLM   51/60      Provides the Integrated ATA RAID Management
                               Utility v4.08 (SPY.NLM)
   CP003454.NLM   51         Supports the Compaq Array adapters for NetWare
                               v5.1 (CPQARRAY.HAM)
   CP003455.NLM   60         Supports the Compaq Array adapters for NetWare
                               v6.0 (CPQARRAY.HAM)
   CP003456.NLM   51/60      Provides the Compaq Ultra/Fast/Wide SCSI-2 HAM
                               (CPQSCSI.HAM)
   CP003457.NLM   51/60      Provides the Adaptec Ultra160 Host Adapter 
                               Module (ADPT160M.HAM)
   CP003458.NLM   51/60      Provides the Compaq Fibre Channel Host Adapter 
                               Module (CPQFC.HAM)
   CP003459.NLM   51/60      Provides the hp ProLiant Server Health Driver
                               Tier 1 (CPQHLTH.NLM)
   CP003460.NLM   51/60      Provides the Smart Array Online Configuration
                               Utility (CPQONLIN.NLM)
   CP003461.NLM   51/60      Provides the Compaq Integrated Management Log
                               Viewer (CPQIML.NLM)
   CP003462.NLM   51/60      Provides the hp ProLiant System Bus Driver
                               (Hot-Plug PCI) Support (CPQSBD.NLM)
   CP003463.NLM   51/60      Provides the Compaq Unified RAID driver (CPQRAID.HAM)
   CP003464.NLM   51/60 (NEW)Provides the hp ProLiant CSB-6 ATA-100 IDE RAID
                               Management Utility v7.21 (SPY2.NLM)
   CP003465.NLM   51/60 (NEW)Provides the hp ProLiant CSB-6 Ultra ATA-100 IDE
                               RAID Controller Driver (LSICSB6.HAM)
   CP003466.NLM   51/60 (NEW)Provides the hp 64-Bit/133-MHz Dual Channel Ultra320
                               Adapter Driver (LSPMPTNW.HAM)
   CP003467.NLM   51/60      Provides the Compaq Foundation Agents (CPQHOST.NLM)
   CP003468.NLM   51/60      Provides the HP Server Agents (CPQBSSA.NLM)
   CP003469.NLM   51/60      Provides the HP NIC Agents (CPQNCSA.NLM)
   CP003470.NLM   51/60      Provides the HP ProLiant Storage Agents
                               (CQMGSTOR.NLM)
   CP003471.NLM   51/60      Provides the Compaq Survey Utility (SURVEY.NLM)


51 = NetWare v5.1, NetWare v5.1 w/SP4, NetWare v5.1 w/SP5, NetWare v5.1 SP6
60 = NetWare v6.0, NetWare v6.0 w/SP1, NetWare v6.0 w/SP2, NetWare v6.0 SP3


4.2 New features included in this PSP

In this version of the PSP, minor bug fixes have been made.


4.3 New and updated drivers/components in this PSP

  o New Drivers in this release of the PSP

      > hp ProLiant CSB-6 ATA-100 IDE RAID Management Utility
         CP003464.NLM
          (SPY2.NLM) v7.21
  
      > hp ProLiant CSB-6 ATA-100 IDE_RAID Controller Driver for Novell
         NetWare
         CP003465.NLM
          (LSICSB6.HAM) v6.09i

      > hp 64-Bit/133MHz Dual Channel Ultra320 Adapter for Novell
         NetWare
         CP003466.NLM
          (LSIMPTNW.HAM) v3.04


  o Support for the following adapters and utilities has been updated
           
      > Fast Ethernet Adapter from HP
         CP003441.NLM
          (N100.LAN) from v6.38 to v7.03

      > HP Gigabit Adapter/Module
         CP003442.NLM
          (N1000.LAN) from v2.75 to v6.79d

      > HP NC77xx/NC67xx Gigabit Server Adapter
         CP003443.NLM
          (Q57.LAN) from v2.38 to v6.01

      > HP Virtual Adapter Driver with Advanced Server Features
         CP003444.NLM
          (QASP.LAN) from v2.10 to v2.19

      > hp ProLiant ACPI Platform Support Module for NetWare 6.x
         CP003446.NLM
          (CPQACPI.PSM) from v1.05 to v1.06

      > AMI IDE / ATA / ATAPI UDMA Host Adapter Module Driver 
         for Novell NetWare
         CP003450.NLM
         (MEGAIDE.HAM) no changes
         (\5X\NWPA.NLM) from v3.09 to 3.09b
         (\5X\MM.NLM) from v2.03 to v2.03a

      > NetWare NWPA MegaRIDE HAM Driver (Multi-Processor Enabled)
         for NetWare v6.0
         CP003451.NLM
          (MEGARIDE.HAM) no changes
          (\60\NWPA.NLM) from v3.12 to v3.12b
          (\60\MM.NLM) from v3.01 to v3.01b

      > NetWare NWPA MegaRIDE HAM Driver for NetWare v5.1
         CP003452.NLM
         (MEGARIDE.HAM) no changes
         (\5X\NWPA.NLM) from v3.09 to 3.09b
         (\5X\MM.NLM) from v2.03 to v2.03a

      > Compaq Disk Array Controller Host Adapter Module for 
         NetWare v5.1
         CP003454.NLM
         (CPQARRAY.HAM) no changes
         (\5X\NWPA.NLM) from v3.09 to 3.09b
         (\5X\MM.NLM) from v2.03 to v2.03a
         (CPQSHD.CDM) from v1.58 to v1.59

      > Hewlett-Packard Company Disk Array Controller Host Adapter
         Module for NetWare v6.0
         CP003455.NLM
          (CPQARRAY.HAM) no changes
	  (\60\NWPA.NLM) from v3.12 to v3.12c
          (\60\MM.NLM) from v3.01 to v3.01b
          (CPQSHD.CDM) from v1.58 to v1.59

      > Compaq Ultra/Fast/Wide SCSI-2 HAM
         CP003456.NLM
          (CPQSCSI.HAM) no changes
	  (\60\NWPA.NLM) from v3.12 to v3.12c
          (\60\MM.NLM) from v3.01 to v3.01b
          (\5X\NWPA.NLM) from v3.09 to 3.09b
          (\5X\MM.NLM) from v2.03 to v2.03a
          (CPQSHD.CDM) from v1.58 to v1.59

      > Adaptec Ultra160 Host Adapter Module
         CP003457.NLM
          (ADPT160M.HAM) from v18.20m to v18.30m
	  (\60\NWPA.NLM) from v3.12 to v3.12c
          (\60\MM.NLM) from v3.01 to v3.01b
          (\5X\NWPA.NLM) from v3.09 to 3.09b
          (\5X\MM.NLM) from v2.03 to v2.03a
          (CPQSHD.CDM) from v1.58 to v1.59

      > Compaq Fibre Channel Host Adapter Module
         CP003458.NLM
          (CPQFC.HAM) from v2.53 to v2.54
	  (\60\NWPA.NLM) from v3.12 to v3.12c
          (\60\MM.NLM) from v3.01 to v3.01b
          (CPQSHD.CDM) from v1.58 to v1.59

      > hp ProLiant Server Health Driver Tier 1
         CP003459.NLM
          (CPQHLTH.NLM) from v5.07 to v5.08

      > Smart Array Online Configuration Utility for NetWare
         CP003460.NLM
          (CPQONLIN.NLM) from v2.68 to v2.70

      > hp ProLiant System Bus Driver for PCI Hot Plug
         CP003462.NLM
          (CPQSBD.NLM) from v3.17 to v3.18

      > Compaq Unified RAID driver
         CP003463.NLM
          (CPQRAID.HAM) from v2.07 to v2.08
	  (\60\NWPA.NLM) from v3.12 to v3.12c
          (\60\MM.NLM) from v3.01 to v3.01b
          (\5X\NWPA.NLM) from v3.09 to 3.09b
          (\5X\MM.NLM) from v2.03 to v2.03a
          (CPQSHD.CDM) from v1.58 to v1.59

      > HP Management Agents
         CP003467.NLM, CP003468.NLM, CP003469.NLM, CP003470.NLM
          from v6.30 to v6.40

      > Compaq Survey Utility for NetWare
         CP003471.NLM
          from v2.52 to v2.54



4.4 Drivers removed from this PSP

  o Support for the following adapters and utilities has been removed
    because the equivalent drivers are available on the Novell base media:

   CP003172.NLM   51/60      Compaq Power Subsystem Utility (CPQPOWER.NLM)
   CP003165.NLM   51/60      Compaq Enhanced Integrated Management
                                Utility (CPQEIMD.NLM)
 



5. Software Installation

The PSP can be installed in one of four ways: 

  o  Command-line by CPQDPLOY.NLM (See Section 5.1)

  o  Graphical (NUT-based) by CPQDPLOY.NLM (See Section 5.2)

  o  Command-line by individual package (See Section 5.3)

  o  Graphical (NUT-based) by individual package (See Section 5.4)


5.1 Command Line Deployment Using CPQDPLOY.NLM

Command-line installation using CPQDPLOY.NLM is achieved by passing as
arguments either a bundle file name or component file name to install
along with either the /nui or /s switches.  If one or more components are
passed to CPQDPLOY.NLM, the /nui switch is assumed.  A bundle file name is
of the format BP00XXXX.XML.  A component file name is of the format
CP0XXXXX.NLM.  CPQDPLOY.NLM is capable of installing either one bundle or
one or more components at a time.  A bundle is a HP-tested collection of
component packages which will deploy device drivers, utilities, agents,
or Survey.  See Section 5.6 for information on how to start the deployment
utility with the "no user interface" option.  Regardless of the 
command-line option passed, information about the success/failure of the
installation is logged in the SYS:\ETC\CPQLOG.LOG file.


5.2 Graphical (NUT-based) Deployment using CPQDPLOY.NLM

Graphical installation using CPQDPLOY.NLM can be done by not using the
-s or -nui parameters to CPQDPLOY.NLM.  You may optionally pass the name
of the bundle or component that you want installed.  The deployment selection
screen will show you the currently installed version of the software on your
server (if found), the version that the component package will install, and
a description of the component package.  The following keystrokes are
available on the graphical screen:

F1 = Display Help
F2 = Toggles the force option
F3 = Toggles the reboot option
F4 = Marks/Unmarks all the components in the list
F5 = Marks/Unmarks an individual component or category in the list
F7 = Toggles whether the STARTUP.NCF and AUTOEXEC.NCF files should be modified
F8 = Display more options
F10 = Installs the marked packages
Enter = Shows the component package details and payload information
Esc = Return to the previous screen or exit the deployment utility

Once installation has completed, a component installation status screen will
be displayed showing the results of the installation.  From this screen,
you can press F3 to view the SYS:\ETC\CPQLOG.LOG file or press Enter on a
component to see further details of the installation.  Pressing Escape
prompts the user to terminate the component installer.  If the reboot the
server option has been selected, the server will be rebooted when 'Yes' is
chosen if no components failed installation and at least one component
requires a reboot prior to being activated.


5.3 Command-Line by Individual Package

Command-line installation of an individual component can be done by
typing the name of the component package (ie CP003458) preceded by the
optional LOAD command and either the /nui or /s switches.  An individual
component package file name is of the format CP0XXXXX.NLM.  The individual
component installer is capable of installing a single component at a time.
A component package will deploy device drivers, utilities, agents, or
Survey.  See Section 5.6 for information on how to start the individual
component installer with the "no user interface" option.  Regardless of
the command-line option passed, information about the success/failure of
the installation is logged in the SYS:\ETC\CPQLOG.LOG file.

5.4 Graphical (NUT-based) Deployment by Individual Package

Graphical installation using the individual component installer can be
done by not using the -s or -nui parameters to the component package.
The deployment selection screen will show you the currently installed
version of the component package on your server (if found), the version
that the component package will install, and a description of the
component package.  The following keystrokes are available on the
graphical screen:

F1 = Display Help
F2 = Toggles the force option
F3 = Toggles the reboot option
F4 = Marks/Unmarks the component to be installed
F5 = Marks/Unmarks the component to be installed
F7 = Toggles whether the STARTUP.NCF and AUTOEXEC.NCF files should be modified 
F8 = Display more options
F10 = Installs the marked package
Enter = Shows the component package details and payload information
Esc = Return to the previous screen or exit the deployment utility

Once installation has completed, a component installation status screen will
be displayed showing the results of the installation.  From this screen,
you can press F3 to view the SYS:\ETC\CPQLOG.LOG file or press Enter on the
component to see further details of the installation.  Pressing Escape
prompts the user to terminate the component installer.  If the "Reboot the
Server" option has been selected, the server will be rebooted when 'Yes' is
chosen if:

	- No component failed installation
	- At least one component that successfully installed requires a 
            reboot

If any component fails installation, a reboot does not occur so that the 
cause of the failure can be determined before the changes have been 
activated.


5.5 List of Command-line parameters

NOTE: Parameters can be entered as upper or lower case, with either a
      slash '/' or dash '-' preceding them.  Parameters in parentheses can
      be used in place of the whole word (ie -(h)elp means that either -h,
      -help, /h or /help can be used)

CPQDPLOY command-line parameters:

   <VOLUME:\PATH\>CPQDPLOY [/H[ELP]|/?] [/NUI] [/S[ILENT]] [/R[EBOOT]]
                           [/F[ORCE]] [/NOMODS] 
                           [BP000xxx.XML|CP00xxxx.NLM]

   <VOLUME:\PATH\>CPQDPLOY [-H[ELP]|-?] [-NUI] [-S[ILENT]] [-R[EBOOT]]
                           [-F[ORCE]] [-NOMODS]  
                           [BP000xxx.XML|CP00xxxx.NLM]

    -(h)elp         Show this list of command-line parameters
    -(r)eboot       Reboot if a package installed requires it and no
                    failures occurred
    -(s)ilent       Silent installation means that all messages will be
                    logged to the SYS:\ETC\CPQLOG.LOG file.  No console
                    output or GUI will be shown.
    -nui            No user interface will be displayed.  However, during
                    installation, output will be shown at the system
                    console unless the -(s)ilent option is also used.
    -(f)orce        Force the installation of a package, regardless of
                    software version installed on the server as long as
                    the software prerequisites have been met.
    -nomods	    Made no modifications to the STARTUP.NCF and
 		    AUTOEXEC.NCF files.  The default option (without this
                    parameter) is to make all modifications as needed
		    during the installation of each component package.

NOTE: If one or more components are passed as parameters to CPQDPLOY,
      the -nui switch is assumed.  The -nui switch is required to install
      a bundle without the GUI.


Individual Component command-line parameters:

   <VOLUME:\PATH\>CP00XXXX [/H[ELP]|/?] [/NUI] [/S[ILENT]] [/NOMODS]
                           [/F[ORCE]] [/I] [/G] [/R[EBOOT]] [/xVOL:\PATH]

   <VOLUME:\PATH\>CP00XXXX [-H[ELP]|-?] [-NUI] [-S[ILENT]] [-NOMODS]
                           [-F[ORCE]] [-I] [-G] [-R[EBOOT]] [-xVOL:\PATH]

    -(h)elp         Show this list of command-line parameters
    -(r)eboot       Reboot if a package installed requires it and no
                    failures occurred
    -(s)ilent       Silent installation means that all messages will be
                    logged to the SYS:\ETC\CPQLOG.LOG file.  No console
                    output or GUI will be shown.
    -nui            No user interface will be displayed.  However, during
                    installation, output will be shown at the system
                    console unless the -(s)ilent option is also used.
    -(f)orce        Force the installation of a package, regardless of
                    software version installed on the server as long as
                    the software prerequisites have been met.
    -i              Display the Package Payload information (no
                    installation occurs)
    -g              Display Package Source and Destination information (no
                    installation occurs)
    -xVol:\Path     Extract the contents of the package to the directory
                    pointed to by Vol:\Path.  Note that there is no space
                    between the x and the path.  If VOL:\Path does not
                    exist, an attempt is made to create the Path.  An
                    invalid volume and/or path will be ignored and the
                    extraction terminated.
    -nomods	    Made no modifications to the STARTUP.NCF and
 		    AUTOEXEC.NCF files.  The default option (without this
                    parameter) is to make all modifications as needed
		    during the installation of each component package.


5.6 Installation Examples

o Normal program execution to deploy a bundle of components for NetWare v5.1.
  The deployment utility will expect the bundle file and all bundles to be
  in the directory which it was called from.  If a bundle file is not found,
  you will be prompted for the path to a bundle file.

  SYS:\DEPLOY\CPQDPLOY

o Using CPQDPLOY to deploy a bundle

  LOAD SYS:\DEPLOY\CPQDPLOY BP000163.XML

o Using the force option for CPQDPLOY.NLM

  LOAD SYS:\DEPLOY\CPQDPLOY -f

o Using the "no user interface" option (No GUI)

  LOAD SYS:\DEPLOY\CPQDPLOY -nui

o Using the silent option (no command-line or GUI output)

  LOAD SYS:\DEPLOY\CPQDPLOY -s

o Using the silent option and the force option

  LOAD SYS:\DEPLOY\CPQDLOY -s -f

o Installing a single component with GUI

  LOAD SYS:\DEPLOY\CP003456

o Installing a single component with force and "no user interface" options

  LOAD SYS:\DEPLOY\CP003470 -f -nui

o Extracting a components contents to another directory

  LOAD SYS:\DEPLOY\CP003454 -xSYS:\TEMP

o Install the contents of a package after extracting a components contents
  to another directory

  LOAD SYS:\TEMP\CPQSETUP

o Determining a components contents without extracting

  LOAD SYS:\DEPLOY\CP003464 -i

o Determining the source directory, destination directory and primary NLM
  that will be installed by the component package

  LOAD SYS:\DEPLOY\CP003468 -g

o Deploying a single component from the deployment utility with force option

  LOAD SYS:\DEPLOY\CPQDPLOY CP003461.NLM -f



6. Log files

During PSP installation an installation log file is generated that contains
more detailed information about the installation than is displayed by
the CPQDPLOY.NLM deployment manager status screen.  The log file is useful
in determining why a particular component failed to install properly.
Each component writes to the installation log file that resides at the
following location:

                 SYS:\ETC\CPQLOG.LOG

To view the installation log file from within the CPQDPLOY.NLM Installation
Status screen, press the F3 key.

To clear the installation log file while it is displayed in the CPQDPLOY.NLM
Installation Status screen, press the F2 key.

The installation log file can also be displayed using any text editor.



7. FAQ

Issue:      I used the /r flag to reboot the server, one of the packages
            installed required a reboot, but the server did not reboot.  What
            is happening?
Resolution: If any of the packages chosen for installation fails the
            installation, a reboot will not occur.  This is so the
            administrator can examine a server to determine and resolve a
            software installation failure before activating any changes.

Issue:      When I examine the package contents, the version of the driver
            in the package is newer than what I have on my server.  However,
            one of the support files is older than the version that is
            contained in the package.  What happens during installation?
Resolution: Each keyfile within a package is version checked (and date 
            checked for non-NLM files) before the file is installed on 
            the server.  If the keyfile in the package is newer than the  
            file on the server, then all files in the package will be 
            installed.  If the keyfile version is the same as or older 
            than the currently installed version, none of the files in
            the component are installed unless the user chooses the force
            option.
*NOTE:      If the /force flag is used, then no version checking is done.
            All files in the package will be installed even if one of
            the files on the server is newer than the one in the package.
            However, OS dependencies are maintained.  For instance, the
            CPQACPI.PSM, which is only supported on NetWare v6.0, will not
            be installed on a server running NetWare v5.1, even if
            the /force flag is used.

Issue:      When I install a driver, then run the installation utility a
            second time before rebooting the server, the version shown in
            the installation utility does not match the version loaded
            via the MODULES console command.
Resolution: Once an installation has occurred, the installation utility
            will check against the installed version on the fixed disk.
            Even if the version loaded is different, the version compared
            against for installations is the version on the physical media.

Issue:      When I do a command-line install and pass the /r parameter, the
            server does not reboot.
Resolution: Normally this occurs because either the version of the software
            to be installed is the same or older than the version installed
            on the server or a failure occurred during the installation
            (such as a prerequisite was not met).  Check the 
            SYS:\ETC\CPQLOG.LOG file to determine the cause of the failure.

Issue:      When I choose the force installation, some packages are not
            installed.
Resolution: The force option will only cause packages to install when
            the software prerequisites for the package have been met.
            If the software prerequisites for a package have not been met,
            the package installation will fail.  In a future release of
            the PSP, an option will be provided to allow installation even
            if the software prerequisites that a package requires are not
            met.

Issue:      During installation, I get error messages about unable to read
            xxx from an XML file or an Error 10010 ... message.
Resolution: This is normally caused by a corrupted package, which
            normally occurs during download.  If a package XML file cannot
            be parsed correctly, the installation of that package will
            terminate with an error such as the above.  To resolve this
            issue, try downloading the package again from
            http://www.hp.com.

Issue:      When I start the PSP with CPQDPLOY.NLM, I get a prompt asking
            me to 'Enter a path to a supported bundle XML file'.
Resolution: This is caused by having CPQDPLOY.NLM in a directory without
            a valid bundle file.  A valid bundle file is a bundle file
            of the format BP000xxx.XML.

Issue:      When upgrading from NetWare v5.x to NetWare v6.0, I get
            an error message during the start of the installation where
            NWPA.NLM is reporting symbols missing for kResume and kSuspend.
Resolution: This is caused by an older version of NWPA.NLM being left in
            the C:\NWUPDATE directory from a previous installation.  The
            above symbols were removed from the kernel in NetWare v6.0.
            To resolve the issue, remove the older NWPA.NLM from the
            C:\NWUPDATE directory.


-----------------------------------------------------------------------------

Copyright 2000-2003 Hewlett-Packard Development Company, L.P.
Hewlett-Packard Company shall not be liable for technical or editorial
errors or omissions contained herein. The information in this document is
provided "as is" without warranty of any kind and is subject to change
without notice. The warranties for HP products are set forth in the
express limited warranty statements accompanying such products. Nothing
herein should be construed as constituting an additional warranty.

Confidential computer software. Valid license from HP required for
possession, use or copying. Consistent with FAR 12.211 and 12.212,
Commercial Computer Software, Computer Software Documentation, and
Technical Data for Commercial Items are licensed to the U.S. Government
under vendor's standard commercial license.
