Connected: An Internet Encyclopedia
RFC 1906 - 7. Proxy to SNMPv1

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1906
Prev: 6.2. Well-known Values
Next: 8. Serialization using the Basic Encoding Rules

### 7. Proxy to SNMPv1

In order to provide proxy to SNMPv1 [8], it may be useful to define a transport domain, rfc1157Domain, which indicates the transport mapping for SNMP messages as defined in RFC 1157. Section 3.1 of [9] specifies the behavior of the proxy agent.

Next: 8. Serialization using the Basic Encoding Rules

Connected: An Internet Encyclopedia
RFC 1906 - 7. Proxy to SNMPv1