Connected: An Internet Encyclopedia
RFC 1661 - 3.1. Overview

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1661
Up: 3. PPP Link Operation
Prev: 3. PPP Link Operation
Next: 3.2. Phase Diagram

### 3.1. Overview

In order to establish communications over a point-to-point link, each end of the PPP link MUST first send LCP packets to configure and test the data link. After the link has been established, the peer MAY be authenticated.

Then, PPP MUST send NCP packets to choose and configure one or more network-layer protocols. Once each of the chosen network-layer protocols has been configured, datagrams from each network-layer protocol can be sent over the link.

The link will remain configured for communications until explicit LCP or NCP packets close the link down, or until some external event occurs (an inactivity timer expires or network administrator intervention).

Next: 3.2. Phase Diagram

Connected: An Internet Encyclopedia
RFC 1661 - 3.1. Overview