Connected: An Internet Encyclopedia
RFC 1771 - 6.3 Reducing route flapping

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1771
Up: Appendix 6. Implementation Recommendations
Prev: 6.2 Processing Messages on a Stream Protocol
Next: 6.4 BGP Timers

### 6.3 Reducing route flapping

To avoid excessive route flapping a BGP speaker which needs to withdraw a destination and send an update about a more specific or less specific route shall combine them into the same UPDATE message.

Next: 6.4 BGP Timers

Connected: An Internet Encyclopedia
RFC 1771 - 6.3 Reducing route flapping