Connected: An Internet Encyclopedia
RFC 1157 - 3.2.6.3.4. ipRoutingTable Object Type Names

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1157
Up: 3. The SNMP Architecture
Up: 3.2. Elements of the Architecture
Up: 3.2.6. Form and Meaning of References to Managed Objects
Up: 3.2.6.3. Identification of Object Instances
Prev: 3.2.6.3.3. ipAddrTable Object Type Names
Next: 3.2.6.3.5. tcpConnTable Object Type Names

### 3.2.6.3.4. ipRoutingTable Object Type Names

The name of an IP route, x, is the OBJECT IDENTIFIER of the form a.b.c.d such that a.b.c.d is the value (in the familiar "dot" notation) of that instance of the ipRouteDest object type associated with x.

For each object type, t, for which the defined name, n, has a prefix of ipRoutingEntry, an instance, i, of t is named by an OBJECT IDENTIFIER of the form n.y, where y is the name of the IP route about which i represents information.

For example, suppose one wanted to find the next hop of an entry in the IP routing table associated with the destination of 89.1.1.42. Accordingly, ipRouteNextHop.89.1.1.42 would identify the desired instance.

Next: 3.2.6.3.5. tcpConnTable Object Type Names

Connected: An Internet Encyclopedia
RFC 1157 - 3.2.6.3.4. ipRoutingTable Object Type Names