Connected: An Internet Encyclopedia
RFC 1906 - 4.1. Serialization

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1906
Up: 4. SNMPv2 over OSI
Prev: 4. SNMPv2 over OSI
Next: 4.2. Well-known Values

### 4.1. Serialization

Each instance of a message is serialized onto a single TSDU [3,4] for the OSI Connectionless-mode Transport Service (CLTS), using the algorithm specified in Section 8.

Next: 4.2. Well-known Values

Connected: An Internet Encyclopedia
RFC 1906 - 4.1. Serialization