Connected: An Internet Encyclopedia
RFC 1906 - 3.1. Serialization

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1906
Up: 3. SNMPv2 over UDP
Prev: 3. SNMPv2 over UDP
Next: 3.2. Well-known Values

### 3.1. Serialization

Each instance of a message is serialized (i.e., encoded according to the convention of [1]) onto a single UDP[2] datagram, using the algorithm specified in Section 8.

Next: 3.2. Well-known Values

Connected: An Internet Encyclopedia
RFC 1906 - 3.1. Serialization