Connected: An Internet Encyclopedia
RFC 1772 - 9.3 TCP Properties

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1772
Up: 9. Operations over Switched Virtual Circuits
Prev: 9.2 Circuit Manager Properties
Next: 9.4 Combined Properties

### 9.3 TCP Properties

A small modification must be made to TCP to process internal notifications from the circuit manager:

- DEAD: Flush transmit queue and abort TCP connection.

- UP: Transmit any queued data or allow an outgoing TCP call to proceed.

Next: 9.4 Combined Properties

Connected: An Internet Encyclopedia
RFC 1772 - 9.3 TCP Properties