Connected: An Internet Encyclopedia
RFC 1902 - 8. Mapping of the NOTIFICATION-TYPE macro

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1902
Prev: 7.11. Usage Example
Next: 8.1. Mapping of the OBJECTS clause

### 8. Mapping of the NOTIFICATION-TYPE macro

The NOTIFICATION-TYPE macro is used to define the information contained within an unsolicited transmission of management information (i.e., within either a SNMPv2-Trap-PDU or InformRequest- PDU). It should be noted that the expansion of the NOTIFICATION-TYPE macro is something which conceptually happens during implementation and not during run-time.

8.1. Mapping of the OBJECTS clause
8.2. Mapping of the STATUS clause
8.3. Mapping of the DESCRIPTION clause
8.4. Mapping of the REFERENCE clause
8.5. Mapping of the NOTIFICATION-TYPE value
8.6. Usage Example

Next: 8.1. Mapping of the OBJECTS clause

Connected: An Internet Encyclopedia
RFC 1902 - 8. Mapping of the NOTIFICATION-TYPE macro