Connected: An Internet Encyclopedia
RFC 1907 - 2.4. Information for Notifications

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1907
Up: 2. Definitions
Prev: 2.2. The SNMP Group
Next: 2.4.1. Well-known Traps

### 2.4. Information for Notifications

    -- information for notifications
    --
    -- a collection of objects which allow the SNMPv2 entity, when
    -- acting in an agent role, to be configured to generate
    -- SNMPv2-Trap-PDUs.

    snmpTrap       OBJECT IDENTIFIER ::= { snmpMIBObjects 4 }

    snmpTrapOID OBJECT-TYPE
        SYNTAX     OBJECT IDENTIFIER
        MAX-ACCESS accessible-for-notify
        STATUS     current
        DESCRIPTION
                "The authoritative identification of the notification
                currently being sent.  This variable occurs as the second
                varbind in every SNMPv2-Trap-PDU and InformRequest-PDU."
        ::= { snmpTrap 1 }

    --  ::= { snmpTrap 2 }   this OID is obsolete

    snmpTrapEnterprise OBJECT-TYPE
        SYNTAX     OBJECT IDENTIFIER
        MAX-ACCESS accessible-for-notify
        STATUS     current
        DESCRIPTION
                "The authoritative identification of the enterprise
                associated with the trap currently being sent.  When a
                SNMPv2 proxy agent is mapping an RFC1157 Trap-PDU into a
                SNMPv2-Trap-PDU, this variable occurs as the last varbind."
        ::= { snmpTrap 3 }

    --  ::= { snmpTrap 4 }   this OID is obsolete

2.4.1. Well-known Traps

Next: 2.4.1. Well-known Traps

Connected: An Internet Encyclopedia
RFC 1907 - 2.4. Information for Notifications