Connected: An Internet Encyclopedia
RFC 793 - 3.6. Precedence and Security

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 793
Up: 3. FUNCTIONAL SPECIFICATION
Prev: 3.5. Closing a Connection
Next: 3.7. Data Communication

### 3.6. Precedence and Security

The intent is that connection be allowed only between ports operating with exactly the same security and compartment values and at the higher of the precedence level requested by the two ports.

The precedence and security parameters used in TCP are exactly those defined in the Internet Protocol (IP) [2]. Throughout this TCP specification the term "security/compartment" is intended to indicate the security parameters used in IP including security, compartment, user group, and handling restriction.

A connection attempt with mismatched security/compartment values or a lower precedence value must be rejected by sending a reset. Rejecting a connection due to too low a precedence only occurs after an acknowledgment of the SYN has been received.

Note that TCP modules which operate only at the default value of precedence will still have to check the precedence of incoming segments and possibly raise the precedence level they use on the connection.

The security paramaters may be used even in a non-secure environment (the values would indicate unclassified data), thus hosts in non-secure environments must be prepared to receive the security parameters, though they need not send them.

Next: 3.7. Data Communication

Connected: An Internet Encyclopedia
RFC 793 - 3.6. Precedence and Security