Connected: An Internet Encyclopedia
RFC 1122 - 4.1.1 INTRODUCTION

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1122
Up: 4. TRANSPORT PROTOCOLS
Up: 4.1 USER DATAGRAM PROTOCOL -- UDP
Prev: 4.1 USER DATAGRAM PROTOCOL -- UDP
Next: 4.1.2 PROTOCOL WALK-THROUGH

### 4.1.1 INTRODUCTION

The User Datagram Protocol UDP [UDP:1] offers only a minimal transport service -- non-guaranteed datagram delivery -- and gives applications direct access to the datagram service of the IP layer. UDP is used by applications that do not require the level of service of TCP or that wish to use communications services (e.g., multicast or broadcast delivery) not available from TCP.

UDP is almost a null protocol; the only services it provides over IP are checksumming of data and multiplexing by port number. Therefore, an application program running over UDP must deal directly with end-to-end communication problems that a connection-oriented protocol would have handled -- e.g., retransmission for reliable delivery, packetization and reassembly, flow control, congestion avoidance, etc., when these are required. The fairly complex coupling between IP and TCP will be mirrored in the coupling between UDP and many applications using UDP.

Next: 4.1.2 PROTOCOL WALK-THROUGH

Connected: An Internet Encyclopedia
RFC 1122 - 4.1.1 INTRODUCTION