Connected: An Internet Encyclopedia
RFC 1832 - 3.6 Floating-point

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1832
Up: 3. XDR DATA TYPES
Prev: 3.5 Hyper Integer and Unsigned Hyper Integer
Next: 3.7 Double-precision Floating-point

### 3.6 Floating-point

The standard defines the floating-point data type "float" (32 bits or 4 bytes). The encoding used is the IEEE standard for normalized single-precision floating-point numbers [3]. The following three fields describe the single-precision floating-point number:

          S: The sign of the number.  Values 0 and 1 represent positive and
             negative, respectively.  One bit.

          E: The exponent of the number, base 2.  8 bits are devoted to this
             field.  The exponent is biased by 127.

          F: The fractional part of the number's mantissa, base 2.  23 bits
             are devoted to this field.

Therefore, the floating-point number is described by:

             (-1)**S * 2**(E-Bias) * 1.F

It is declared as follows:

             float identifier;

             +-------+-------+-------+-------+
             |byte 0 |byte 1 |byte 2 |byte 3 |              SINGLE-PRECISION
             S|   E   |           F          |         FLOATING-POINT NUMBER
             +-------+-------+-------+-------+
             1|<- 8 ->|<-------23 bits------>|
             <------------32 bits------------>

Just as the most and least significant bytes of a number are 0 and 3, the most and least significant bits of a single-precision floating- point number are 0 and 31. The beginning bit (and most significant bit) offsets of S, E, and F are 0, 1, and 9, respectively. Note that these numbers refer to the mathematical positions of the bits, and NOT to their actual physical locations (which vary from medium to medium).

The IEEE specifications should be consulted concerning the encoding for signed zero, signed infinity (overflow), and denormalized numbers (underflow) [3]. According to IEEE specifications, the "NaN" (not a number) is system dependent and should not be interpreted within XDR as anything other than "NaN".

Next: 3.7 Double-precision Floating-point

Connected: An Internet Encyclopedia
RFC 1832 - 3.6 Floating-point