Connected: An Internet Encyclopedia
RFC 1945 - 9.4 Client Error 4xx

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1945
Up: 9. Status Code Definitions
Prev: 9.3 Redirection 3xx
Next: 9.5 Server Error 5xx

### 9.4 Client Error 4xx

The 4xx class of status code is intended for cases in which the client seems to have erred. If the client has not completed the request when a 4xx code is received, it should immediately cease sending data to the server. Except when responding to a HEAD request, the server should include an entity containing an explanation of the error situation, and whether it is a temporary or permanent condition. These status codes are applicable to any request method.

Note: If the client is sending data, server implementations on TCP should be careful to ensure that the client acknowledges receipt of the packet(s) containing the response prior to closing the input connection. If the client continues sending data to the server after the close, the server's controller will send a reset packet to the client, which may erase the client's unacknowledged input buffers before they can be read and interpreted by the HTTP application.

#### 400 Bad Request

The request could not be understood by the server due to malformed syntax. The client should not repeat the request without modifications.

#### 401 Unauthorized

The request requires user authentication. The response must include a WWW-Authenticate header field (Section 10.16) containing a challenge applicable to the requested resource. The client may repeat the request with a suitable Authorization header field (Section 10.2). If the request already included Authorization credentials, then the 401 response indicates that authorization has been refused for those credentials. If the 401 response contains the same challenge as the prior response, and the user agent has already attempted authentication at least once, then the user should be presented the entity that was given in the response, since that entity may include relevant diagnostic information. HTTP access authentication is explained in Section 11.

#### 403 Forbidden

The server understood the request, but is refusing to fulfill it. Authorization will not help and the request should not be repeated. If the request method was not HEAD and the server wishes to make public why the request has not been fulfilled, it should describe the reason for the refusal in the entity body. This status code is commonly used when the server does not wish to reveal exactly why the request has been refused, or when no other response is applicable.

#### 404 Not Found

The server has not found anything matching the Request-URI. No indication is given of whether the condition is temporary or permanent. If the server does not wish to make this information available to the client, the status code 403 (forbidden) can be used instead.

Next: 9.5 Server Error 5xx

Connected: An Internet Encyclopedia
RFC 1945 - 9.4 Client Error 4xx