Connected: An Internet Encyclopedia
RFC 1812 - 8.3 Standard MIBS

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Up: 8. APPLICATION LAYER - NETWORK MANAGEMENT PROTOCOLS
Prev: 8.2 Community Table
Next: 8.4 Vendor Specific MIBS

### 8.3 Standard MIBS

All MIBS relevant to a router's configuration are to be implemented. To wit:

- The System, Interface, IP, ICMP, and UDP groups of MIB-II [MGT:2] MUST be implemented.

- The Interface Extensions MIB [MGT:18] MUST be implemented.

- The IP Forwarding Table MIB [MGT:20] MUST be implemented.

- If the router implements TCP (e.g., for Telnet) then the TCP group of MIB-II [MGT:2] MUST be implemented.

- If the router implements EGP then the EGP group of MIB-II [MGT:2] MUST be implemented.

- If the router supports OSPF then the OSPF MIB [MGT:14] MUST be implemented.

- If the router supports BGP then the BGP MIB [MGT:15] MUST be implemented.

- If the router has Ethernet, 802.3, or StarLan interfaces then the Ethernet-Like MIB [MGT:6] MUST be implemented.

- If the router has 802.4 interfaces then the 802.4 MIB [MGT:7] MUST be implemented.

- If the router has 802.5 interfaces then the 802.5 MIB [MGT:8] MUST be implemented.

- If the router has FDDI interfaces that implement ANSI SMT 7.3 then the FDDI MIB [MGT:9] MUST be implemented.

- If the router has FDDI interfaces that implement ANSI SMT 6.2 then the FDDI MIB [MGT:29] MUST be implemented.

- If the router has interfaces that use V.24 signalling, such as RS- 232, V.10, V.11, V.35, V.36, or RS-422/423/449, then the RS-232 [MGT:10] MIB MUST be implemented.

- If the router has T1/DS1 interfaces then the T1/DS1 MIB [MGT:16] MUST be implemented.

- If the router has T3/DS3 interfaces then the T3/DS3 MIB [MGT:17] MUST be implemented.
- If the router has SMDS interfaces then the SMDS Interface Protocol MIB [MGT:19] MUST be implemented.

- If the router supports PPP over any of its interfaces then the PPP MIBs [MGT:11], [MGT:12], and [MGT:13] MUST be implemented.

- If the router supports RIP Version 2 then the RIP Version 2 MIB [MGT:21] MUST be implemented.

- If the router supports X.25 over any of its interfaces then the X.25 MIBs [MGT:22, MGT:23 and MGT:24] MUST be implemented.

Next: 8.4 Vendor Specific MIBS

Connected: An Internet Encyclopedia
RFC 1812 - 8.3 Standard MIBS