Connected: An Internet Encyclopedia
RFC 1583 - E.4 TOS encoding updated

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1583
Up: E. Differences from RFC 1247
Prev: E.3 Obsoleting LSInfinity in router links advertisements
Next: E.5 Summarizing routes into transit areas

### E.4 TOS encoding updated

The encoding of TOS in OSPF link state advertisements has been updated to reflect the new TOS value (minimize monetary cost) defined by [RFC 1349]. The OSPF encoding is defined in Section 12.3, which is identical in content to Section A.5 of [RFC 1349].

Next: E.5 Summarizing routes into transit areas

Connected: An Internet Encyclopedia
RFC 1583 - E.4 TOS encoding updated