Connected: An Internet Encyclopedia
RFC 977 - 2.4.3. General Responses

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 977
Up: 2. The NNTP Specification
Up: 2.4. Responses
Prev: 2.4.2. Status Responses
Next: 3. Command and Response Details

### 2.4.3. General Responses

The following is a list of general response codes that may be sent by the NNTP server. These are not specific to any one command, but may be returned as the result of a connection, a failure, or some unusual condition.

In general, 1xx codes may be ignored or displayed as desired; code 200 or 201 is sent upon initial connection to the NNTP server depending upon posting permission; code 400 will be sent when the NNTP server discontinues service (by operator request, for example); and 5xx codes indicate that the command could not be performed for some unusual reason.

          100 help text
          190
            through
          199 debug output

          200 server ready - posting allowed
          201 server ready - no posting allowed

          400 service discontinued

          500 command not recognized
          501 command syntax error
          502 access restriction or permission denied
          503 program fault - command not performed

Next: 3. Command and Response Details

Connected: An Internet Encyclopedia
RFC 977 - 2.4.3. General Responses