Connected: An Internet Encyclopedia
RFC 1421 - 4.6.2 Encapsulated Header Fields Normally Per-Message

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1421
Up: 4. Processing of Messages
Up: 4.6 Summary of Encapsulated Header Fields
Prev: 4.6.1.3 DEK-Info Field
Next: 4.6.2.1 Originator-ID Fields

### 4.6.2 Encapsulated Header Fields Normally Per-Message

This group of encapsulated header fields contains fields which ordinarily occur no more than once per message. Depending on the key management option(s) employed, some of these fields may be absent from some messages.

4.6.2.1 Originator-ID Fields

4.6.2.1.1 Originator-ID-Asymmetric Field
4.6.2.1.2 Originator-ID-Symmetric Field

4.6.2.2 Originator-Certificate Field
4.6.2.3 MIC-Info Field

Next: 4.6.2.1 Originator-ID Fields

Connected: An Internet Encyclopedia
RFC 1421 - 4.6.2 Encapsulated Header Fields Normally Per-Message