Connected: An Internet Encyclopedia
RFC 1905 - 2.6. Transport Mappings

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1905
Up: 2. Overview
Prev: 2.5. Message Sizes
Next: 3. Definitions

### 2.6. Transport Mappings

It is important to note that the exchange of SNMPv2 messages requires only an unreliable datagram service, with every message being entirely and independently contained in a single transport datagram. Specific transport mappings and encoding rules are specified elsewhere [5]. However, the preferred mapping is the use of the User Datagram Protocol [6].

Next: 3. Definitions

Connected: An Internet Encyclopedia
RFC 1905 - 2.6. Transport Mappings