Connected: An Internet Encyclopedia
RFC 951 - 7.4. Server/Gateway Receives BOOTREPLY

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 951
Up: 7. Packet Processing
Prev: 7.3. Server Receives BOOTREQUEST
Next: 7.5. Client Reception

### 7.4. Server/Gateway Receives BOOTREPLY

[UDP checksum.] If 'yiaddr' (your [the client's] IP address) refers to one of our cables, use one of the 'Egg' methods above to forward it to the client. Be sure to send it to the 'BOOTP client' UDP destination port.

Next: 7.5. Client Reception

Connected: An Internet Encyclopedia
RFC 951 - 7.4. Server/Gateway Receives BOOTREPLY