Connected: An Internet Encyclopedia
RFC 1421 - 4.6.1.1.1 ENCRYPTED

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1421
Up: 4. Processing of Messages
Up: 4.6 Summary of Encapsulated Header Fields
Up: 4.6.1 Per-Message Encapsulated Header Fields
Up: 4.6.1.1 Proc-Type Field
Prev: 4.6.1.1 Proc-Type Field
Next: 4.6.1.1.2 MIC-ONLY

### 4.6.1.1.1 ENCRYPTED

The "ENCRYPTED" specifier signifies that confidentiality, authentication, integrity, and (given use of asymmetric key management) non-repudiation of origin security services have been applied to a PEM message's encapsulated text. ENCRYPTED messages require a "DEK-Info:" field and individual Recipient-ID and "Key- Info:" fields for all message recipients.

Next: 4.6.1.1.2 MIC-ONLY

Connected: An Internet Encyclopedia
RFC 1421 - 4.6.1.1.1 ENCRYPTED