Connected: An Internet Encyclopedia
RFC 1812 - 5.3.12.2 When a Router Starts Forwarding

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Up: 5. INTERNET LAYER - FORWARDING
Up: 5.3 SPECIFIC ISSUES
Up: 5.3.12 State Changes
Prev: 5.3.12.1 When a Router Ceases Forwarding
Next: 5.3.12.3 When an Interface Fails or is Disabled

### 5.3.12.2 When a Router Starts Forwarding

When a router begins forwarding, it SHOULD expedite the sending of new routing information to all routers with which it normally exchanges routing information.

Next: 5.3.12.3 When an Interface Fails or is Disabled

Connected: An Internet Encyclopedia
RFC 1812 - 5.3.12.2 When a Router Starts Forwarding