Connected: An Internet Encyclopedia
RFC 1421 - 4.6.1.2 Content-Domain Field

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1421
Up: 4. Processing of Messages
Up: 4.6 Summary of Encapsulated Header Fields
Up: 4.6.1 Per-Message Encapsulated Header Fields
Prev: 4.6.1.1.4 CRL
Next: 4.6.1.3 DEK-Info Field

### 4.6.1.2 Content-Domain Field

The "Content-Domain:" encapsulated header field describes the type of content which is represented within a PEM message's encapsulated text. It carries one string argument, whose value is defined as "RFC822" to indicate processing of RFC-822 mail as defined in this specification. It is anticipated that additional "Content-Domain:" values will be defined subsequently, in additional or successor documents to this specification. Only one "Content-Domain:" field occurs in a PEM message; this field is the PEM message's second encapsulated header field, immediately following the "Proc-Type:" field.

Next: 4.6.1.3 DEK-Info Field

Connected: An Internet Encyclopedia
RFC 1421 - 4.6.1.2 Content-Domain Field