Connected: An Internet Encyclopedia
RFC 826 - Definitions

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 826
Prev: Motivation
Next: Packet format

### Definitions

Define the following for referring to the values put in the TYPE field of the Ethernet packet header:

    	ether_type$XEROX_PUP,
    	ether_type$DOD_INTERNET,
    	ether_type$CHAOS,

and a new one:

    	ether_type$ADDRESS_RESOLUTION.

Also define the following values (to be discussed later):

    	ares_op$REQUEST (= 1, high byte transmitted first) and
    	ares_op$REPLY   (= 2),

and

    	ares_hrd$Ethernet (= 1).

Next: Packet format

Connected: An Internet Encyclopedia
RFC 826 - Definitions