Connected: An Internet Encyclopedia
RFC 1945 - D.2.1 Accept

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1945
Up: D. Additional Features
Up: D.2 Additional Header Field Definitions
Prev: D.2 Additional Header Field Definitions
Next: D.2.2 Accept-Charset

### D.2.1 Accept

The Accept request-header field can be used to indicate a list of media ranges which are acceptable as a response to the request. The asterisk "*" character is used to group media types into ranges, with "*/*" indicating all media types and "type/*" indicating all subtypes of that type. The set of ranges given by the client should represent what types are acceptable given the context of the request.

Next: D.2.2 Accept-Charset

Connected: An Internet Encyclopedia
RFC 1945 - D.2.1 Accept