Connected: An Internet Encyclopedia
RFC 1122 - 2.3.1 Trailer Protocol Negotiation

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1122
Up: 2. LINK LAYER
Up: 2.3 SPECIFIC ISSUES
Prev: 2.3 SPECIFIC ISSUES
Next: 2.3.2 Address Resolution Protocol -- ARP

### 2.3.1 Trailer Protocol Negotiation

The trailer protocol [LINK:1] for link-layer encapsulation MAY be used, but only when it has been verified that both systems (host or gateway) involved in the link-layer communication implement trailers. If the system does not dynamically negotiate use of the trailer protocol on a per-destination basis, the default configuration MUST disable the protocol.

DISCUSSION:

  The trailer protocol is a link-layer encapsulation technique that rearranges the data contents of packets sent on the physical network. In some cases, trailers improve the throughput of higher layer protocols by reducing the amount of data copying within the operating system. Higher layer protocols are unaware of trailer use, but both the sending and receiving host MUST understand the protocol if it is used.

  Improper use of trailers can result in very confusing symptoms. Only packets with specific size attributes are encapsulated using trailers, and typically only a small fraction of the packets being exchanged have these attributes. Thus, if a system using trailers exchanges packets with a system that does not, some packets disappear into a black hole while others are delivered successfully.

IMPLEMENTATION:

  On an Ethernet, packets encapsulated with trailers use a distinct Ethernet type [LINK:1], and trailer negotiation is performed at the time that ARP is used to discover the link-layer address of a destination system. Specifically, the ARP exchange is completed in the usual manner using the normal IP protocol type, but a host that wants to speak trailers will send an additional "trailer ARP reply" packet, i.e., an ARP reply that specifies the trailer encapsulation protocol type but otherwise has the format of a normal ARP reply. If a host configured to use trailers receives a trailer ARP reply message from a remote machine, it can add that machine to the list of machines that understand trailers, e.g., by marking the corresponding entry in the ARP cache.

  Hosts wishing to receive trailer encapsulations send trailer ARP replies whenever they complete exchanges of normal ARP messages for IP. Thus, a host that received an ARP request for its IP protocol address would send a trailer ARP reply in addition to the normal IP ARP reply; a host that sent the IP ARP request would send a trailer ARP reply when it received the corresponding IP ARP reply. In this way, either the requesting or responding host in an IP ARP exchange may request that it receive trailer encapsulations.

  This scheme, using extra trailer ARP reply packets rather than sending an ARP request for the trailer protocol type, was designed to avoid a continuous exchange of ARP packets with a misbehaving host that, contrary to any specification or common sense, responded to an ARP reply for trailers with another ARP reply for IP. This problem is avoided by sending a trailer ARP reply in response to an IP ARP reply only when the IP ARP reply answers an outstanding request; this is true when the hardware address for the host is still unknown when the IP ARP reply is received. A trailer ARP reply may always be sent along with an IP ARP reply responding to an IP ARP request.

Next: 2.3.2 Address Resolution Protocol -- ARP

Connected: An Internet Encyclopedia
RFC 1122 - 2.3.1 Trailer Protocol Negotiation