Connected: An Internet Encyclopedia
RFC 1812 - 9. APPLICATION LAYER - MISCELLANEOUS PROTOCOLS

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Prev: 8.5 Saving Changes
Next: 9.1 BOOTP

### 9. APPLICATION LAYER - MISCELLANEOUS PROTOCOLS

For all additional application protocols that a router implements, the router MUST be compliant and SHOULD be unconditionally compliant with the relevant requirements of [INTRO:3].

9.1 BOOTP

9.1.1 Introduction
9.1.2 BOOTP Relay Agents

Next: 9.1 BOOTP

Connected: An Internet Encyclopedia
RFC 1812 - 9. APPLICATION LAYER - MISCELLANEOUS PROTOCOLS