Connected: An Internet Encyclopedia
RFC 1812 - 3.3.5.3 IP Control Protocol (IPCP) Options

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Up: 3. LINK LAYER
Up: 3.3 SPECIFIC ISSUES
Up: 3.3.5 Point-to-Point Protocol - PPP
Prev: 3.3.5.2 Link Control Protocol (LCP) Options
Next: 3.3.6 Interface Testing

### 3.3.5.3 IP Control Protocol (IPCP) Options

A router MAY offer to perform IP address negotiation. A router MUST accept a refusal (REJect) to perform IP address negotiation from the peer.

Routers operating at link speeds of 19,200 BPS or less SHOULD implement and offer to perform Van Jacobson header compression. Routers that implement VJ compression SHOULD implement an administrative control enabling or disabling it.

Next: 3.3.6 Interface Testing

Connected: An Internet Encyclopedia
RFC 1812 - 3.3.5.3 IP Control Protocol (IPCP) Options