Connected: An Internet Encyclopedia
RFC 1904 - 4.6. Usage Example

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1904
Up: 4. Mapping of the NOTIFICATION-GROUP macro
Prev: 4.5. Mapping of the NOTIFICATION-GROUP value
Next: 5. Mapping of the MODULE-COMPLIANCE macro

### 4.6. Usage Example

The SNMP Basic Notifications Group [3] is described:

    snmpBasicNotificationsGroup NOTIFICATION-GROUP
        NOTIFICATIONS { coldStart, authenticationFailure }
        STATUS        current
        DESCRIPTION
                "The two notifications which an SNMPv2 entity is required to
                implement."
        ::= { snmpMIBGroups 7 }

According to this invocation, the conformance group named

         { snmpMIBGroups 1 }

contains 2 notifications.

Next: 5. Mapping of the MODULE-COMPLIANCE macro

Connected: An Internet Encyclopedia
RFC 1904 - 4.6. Usage Example