Connected: An Internet Encyclopedia
RFC 1700 - pronet80-type-numbers

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1700

Search: |  | Search Depth: |
Search Type: | String RegEx | Search Options: | NoCase WholeWord

    PRONET 80 TYPE NUMBERS

    Below is the current list of PRONET 80 Type Numbers.  Note: a protocol
    that is on this list does not necessarily mean that there is any
    implementation of it on ProNET.

    Of these, protocols 1, 14, and 20 are the only ones that have ever
    been seen in ARP packets.

    For reference, the header is (one byte/line):

    	destination hardware address
    	source hardware address
    	data link header version (2)
    	data link header protocol number
    	data link header reserved (0)
    	data link header reserved (0)

    Some protocols have been known to tuck stuff in the reserved fields.

    Those who need a protocol number on ProNET-10/80 should contact
    Avri Doria .

    1	IP
    2	IP with trailing headers
    3	Address Resolution Protocol
    4	Proteon HDLC
    5	VAX Debugging Protocol (MIT)
    10	Novell NetWare (IPX and pre-IPX) (old format,
            3 byte trailer)
    11	Vianetix
    12	PUP
    13	Watstar protocol (University of Waterloo)
    14	XNS
    15	Diganostics
    16	Echo protocol (link level)
    17	Banyan Vines
    20	DECnet (DEUNA Emulation)
    21	Chaosnet
    23	IEEE 802.2 or ISO 8802/2 Data Link
    24	Reverse Address Resolution Protocol
    29	TokenVIEW-10
    31	AppleTalk LAP Data Packet
    33	Cornell Boot Server Location Protocol
    34	Novell NetWare IPX (new format, no trailer,
            new XOR checksum)

    []

Connected: An Internet Encyclopedia
RFC 1700 - pronet80-type-numbers