Connected: An Internet Encyclopedia
RFC 1122 - 4.2.2.9 Initial Sequence Number Selection

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1122
Up: 4. TRANSPORT PROTOCOLS
Up: 4.2 TRANSMISSION CONTROL PROTOCOL -- TCP
Up: 4.2.2 PROTOCOL WALK-THROUGH
Prev: 4.2.2.8 TCP Connection State Diagram: RFC-793 Section 3.2, page 23
Next: 4.2.2.10 Simultaneous Open Attempts: RFC-793 Section 3.4, page 32

### 4.2.2.9 Initial Sequence Number Selection: RFC-793 Section 3.3, page 27

A TCP MUST use the specified clock-driven selection of initial sequence numbers.

Next: 4.2.2.10 Simultaneous Open Attempts: RFC-793 Section 3.4, page 32

Connected: An Internet Encyclopedia
RFC 1122 - 4.2.2.9 Initial Sequence Number Selection