Connected: An Internet Encyclopedia
RFC 1452 - 3.1.1. SNMPv2 -> SNMPv1

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1452
Up: 3. Protocol Operations
Up: 3.1. Proxy Agent Behavior
Prev: 3.1. Proxy Agent Behavior
Next: 3.1.2. SNMPv1 -> SNMPv2

### 3.1.1. SNMPv2 -> SNMPv1

When converting requests from a SNMPv2 entity acting in a manager role into requests sent to a SNMPv1 entity acting in an agent role:

1. If a GetRequest-PDU, GetNextRequest-PDU, or SetRequest- PDU is received, then it is passed unaltered by the proxy agent.

2. If a GetBulkRequest-PDU is received, the proxy agent sets the non-repeaters and max-repetitions fields to zero, and sets the tag of the PDU to GetNextRequest-PDU.

Next: 3.1.2. SNMPv1 -> SNMPv2

Connected: An Internet Encyclopedia
RFC 1452 - 3.1.1. SNMPv2 -> SNMPv1