Connected: An Internet Encyclopedia
ICMP Protocol Overview

Top: Connected: An Internet Encyclopedia
Up: Topics
Up: Functions
Up: Transport

Search: |  | Search Depth: |
Search Type: | String RegEx | Search Options: | NoCase WholeWord

### ICMP Protocol Overview

Internet Control Message Protocol (ICMP), documented in RFC 792, is a required protocol tightly integrated with IP. ICMP messages, delivered in IP packets, are used for out-of-band messages related to network operation or mis-operation. Of course, since ICMP uses IP, ICMP packet delivery is unreliable, so hosts can't count on receiving ICMP packets for any network problem. Some of ICMP's functions are to:

- Announce network errors, such as a host or entire portion of the network being unreachable, due to some type of failure. A TCP or UDP packet directed at a port number with no receiver attached is also reported via ICMP.

- Announce network congestion. When a router begins buffering too many packets, due to an inability to transmit them as fast as they are being received, it will generate ICMP Source Quench messages. Directed at the sender, these messages should cause the rate of packet transmission to be slowed. Of course, generating too many Source Quench messages would cause even more network congestion, so they are used sparingly.

- Assist Troubleshooting. ICMP supports an Echo function, which just sends a packet on a round--trip between two hosts. Ping, a common network management tool, is based on this feature. Ping will transmit a series of packets, measuring average round--trip times and computing loss percentages.

- Announce Timeouts. If an IP packet's TTL field drops to zero, the router discarding the packet will often generate an ICMP packet announcing this fact. TraceRoute is a tool which maps network routes by sending packets with small TTL values and watching the ICMP timeout announcements.

Connected: An Internet Encyclopedia
ICMP Protocol Overview