Connected: An Internet Encyclopedia
RFC 1323 - 3.3 The RTTM Mechanism

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1323
Up: 3. RTTM: ROUND-TRIP TIME MEASUREMENT
Prev: 3.2 TCP Timestamps Option
Next: 3.4 Which Timestamp to Echo

### 3.3 The RTTM Mechanism

The timestamp value to be sent in TSval is to be obtained from a (virtual) clock that we call the "timestamp clock". Its values must be at least approximately proportional to real time, in order to measure actual RTT.

The following example illustrates a one-way data flow with segments arriving in sequence without loss. Here A, B, C... represent data blocks occupying successive blocks of sequence numbers, and ACK(A),... represent the corresponding cumulative acknowledgments. The two timestamp fields of the Timestamps option are shown symbolically as <TSval= x,TSecr=y>. Each TSecr field contains the value most recently received in a TSval field.

             TCP  A                                          TCP B

                            <A,TSval=1,TSecr=120> ------>

                 <---- <ACK(A),TSval=127,TSecr=1>

                            <B,TSval=5,TSecr=127> ------>

                 <---- <ACK(B),TSval=131,TSecr=5>

                 . . . . . . . . . . . . . . . . . . . . . .

                            <C,TSval=65,TSecr=131> ------>

                 <---- <ACK(C),TSval=191,TSecr=65>

                            (etc)

The dotted line marks a pause (60 time units long) in which A had nothing to send. Note that this pause inflates the RTT which B could infer from receiving TSecr=131 in data segment C. Thus, in one-way data flows, RTTM in the reverse direction measures a value that is inflated by gaps in sending data. However, the following rule prevents a resulting inflation of the measured RTT:

A TSecr value received in a segment is used to update the averaged RTT measurement only if the segment acknowledges some new data, i.e., only if it advances the left edge of the send window.

Since TCP B is not sending data, the data segment C does not acknowledge any new data when it arrives at B. Thus, the inflated RTTM measurement is not used to update B's RTTM measurement.

Next: 3.4 Which Timestamp to Echo

Connected: An Internet Encyclopedia
RFC 1323 - 3.3 The RTTM Mechanism