Connected: An Internet Encyclopedia
RFC 1812 - 3.3.3 Ethernet and 802.3 Coexistence

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Up: 3. LINK LAYER
Up: 3.3 SPECIFIC ISSUES
Prev: 3.3.2 Address Resolution Protocol - ARP
Next: 3.3.4 Maximum Transmission Unit - MTU

### 3.3.3 Ethernet and 802.3 Coexistence

Routers that can connect to ten megabit Ethernets MUST be compliant and SHOULD be unconditionally compliant with the Ethernet requirements of [INTRO:2].

Next: 3.3.4 Maximum Transmission Unit - MTU

Connected: An Internet Encyclopedia
RFC 1812 - 3.3.3 Ethernet and 802.3 Coexistence