Connected: An Internet Encyclopedia
RFC 1812 - 7.5 FILTERING OF ROUTING INFORMATION

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Up: 7. APPLICATION LAYER - ROUTING PROTOCOLS
Prev: 7.4 STATIC ROUTING
Next: 7.5.1 Route Validation

### 7.5 FILTERING OF ROUTING INFORMATION

Each router within a network makes forwarding decisions based upon information contained within its forwarding database. In a simple network the contents of the database may be configured statically. As the network grows more complex, the need for dynamic updating of the forwarding database becomes critical to the efficient operation of the network.

If the data flow through a network is to be as efficient as possible, it is necessary to provide a mechanism for controlling the propagation of the information a router uses to build its forwarding database. This control takes the form of choosing which sources of routing information should be trusted and selecting which pieces of the information to believe. The resulting forwarding database is a filtered version of the available routing information.

In addition to efficiency, controlling the propagation of routing information can reduce instability by preventing the spread of incorrect or bad routing information.

In some cases local policy may require that complete routing information not be widely propagated.

These filtering requirements apply only to non-SPF-based protocols (and therefore not at all to routers which don't implement any distance vector protocols).

7.5.1 Route Validation
7.5.2 Basic Route Filtering
7.5.3 Advanced Route Filtering

Next: 7.5.1 Route Validation

Connected: An Internet Encyclopedia
RFC 1812 - 7.5 FILTERING OF ROUTING INFORMATION