Connected: An Internet Encyclopedia
RFC 1850 - 3.6. OSPF Host Table

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1850
Up: 3. Definitions
Prev: 3.5. OSPF Address Range Table
Next: 3.7. OSPF Interface Table

### 3.6. OSPF Host Table

    --  OSPF Host Table

    --      The Host/Metric Table indicates what hosts are directly
    --      attached to the Router, and what metrics and types of
    --      service should be advertised for them.

        ospfHostTable OBJECT-TYPE
            SYNTAX   SEQUENCE OF OspfHostEntry
            MAX-ACCESS   not-accessible
            STATUS   current
            DESCRIPTION
               "The list of Hosts, and their metrics, that the
               router will advertise as host routes."
           REFERENCE
              "OSPF Version 2, Appendix C.6  Host route param-
              eters"
          ::= { ospf 6 }

        ospfHostEntry OBJECT-TYPE
            SYNTAX   OspfHostEntry
            MAX-ACCESS   not-accessible
            STATUS   current
            DESCRIPTION
               "A metric to be advertised, for a given type of
               service, when a given host is reachable."
           INDEX { ospfHostIpAddress, ospfHostTOS }
           ::= { ospfHostTable 1 }

    OspfHostEntry ::=
        SEQUENCE {
            ospfHostIpAddress
                IpAddress,
            ospfHostTOS
                TOSType,
            ospfHostMetric
                Metric,
            ospfHostStatus
                RowStatus,
            ospfHostAreaID
                AreaID
                  }

        ospfHostIpAddress OBJECT-TYPE
            SYNTAX   IpAddress
            MAX-ACCESS   read-only
            STATUS   current
            DESCRIPTION
               "The IP Address of the Host."
           REFERENCE
              "OSPF Version 2, Appendix C.6 Host route parame-
              ters"
          ::= { ospfHostEntry 1 }

        ospfHostTOS OBJECT-TYPE
            SYNTAX   TOSType
            MAX-ACCESS   read-only
            STATUS   current
            DESCRIPTION
               "The Type of Service of the route being config-
               ured."
           REFERENCE
              "OSPF Version 2, Appendix C.6 Host route parame-
              ters"
          ::= { ospfHostEntry 2 }

        ospfHostMetric OBJECT-TYPE
            SYNTAX   Metric
            MAX-ACCESS   read-create
            STATUS   current
            DESCRIPTION
               "The Metric to be advertised."
           REFERENCE
              "OSPF Version 2, Appendix C.6 Host route parame-
              ters"
          ::= { ospfHostEntry 3 }

        ospfHostStatus OBJECT-TYPE
            SYNTAX   RowStatus
            MAX-ACCESS   read-create
            STATUS   current
            DESCRIPTION
               "This variable displays the status of  the  en-
               try.  Setting it to 'invalid' has the effect of
               rendering it inoperative.  The internal  effect
               (row removal) is implementation dependent."
           ::= { ospfHostEntry 4 }

        ospfHostAreaID OBJECT-TYPE
            SYNTAX   AreaID
            MAX-ACCESS   read-only
            STATUS   current
            DESCRIPTION
               "The Area the Host Entry is to be found within.
               By  default, the area that a subsuming OSPF in-
               terface is in, or 0.0.0.0"
           REFERENCE
              "OSPF Version 2, Appendix C.2 Area parameters"
          ::= { ospfHostEntry 5 }

Next: 3.7. OSPF Interface Table

Connected: An Internet Encyclopedia
RFC 1850 - 3.6. OSPF Host Table