Connected: An Internet Encyclopedia
RFC 1902 - 11.3. Event Mapping

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1902
Up: 11. Appendix A: de-OSIfying a MIB module
Prev: 11.2.5. Mapping to the REFERENCE clause
Next: 11.3.1. Mapping to the STATUS clause

### 11.3. Event Mapping

Events are modeled as SNMPv2 notifications using NOTIFICATION-TYPE macro. However, recall that SNMPv2 emphasizes trap-directed polling. As such, few, and usually no, notifications, need be defined for any MIB module.

11.3.1. Mapping to the STATUS clause
11.3.2. Mapping to the DESCRIPTION clause
11.3.3. Mapping to the REFERENCE clause

Next: 11.3.1. Mapping to the STATUS clause

Connected: An Internet Encyclopedia
RFC 1902 - 11.3. Event Mapping