Connected: An Internet Encyclopedia
RFC 1123 - 4.1.2.11 FTP Replies: RFC-959 Section 4.2, Page 35

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1123
Up: 4. FILE TRANSFER
Up: 4.1 FILE TRANSFER PROTOCOL -- FTP
Up: 4.1.1 INTRODUCTION
Prev: 4.1.2.10 Telnet End-of-line Code: RFC-959, Page 34
Next: 4.1.2.12 Connections: RFC-959 Section 5.2

### 4.1.2.11 FTP Replies: RFC-959 Section 4.2, Page 35

A Server-FTP MUST send only correctly formatted replies on the control connection. Note that RFC-959 (unlike earlier versions of the FTP spec) contains no provision for a "spontaneous" reply message.

A Server-FTP SHOULD use the reply codes defined in RFC-959 whenever they apply. However, a server-FTP MAY use a different reply code when needed, as long as the general rules of Section 4.2 are followed. When the implementor has a choice between a 4xx and 5xx reply code, a Server-FTP SHOULD send a 4xx (temporary failure) code when there is any reasonable possibility that a failed FTP will succeed a few hours later.

A User-FTP SHOULD generally use only the highest-order digit of a 3-digit reply code for making a procedural decision, to prevent difficulties when a Server-FTP uses non-standard reply codes.

A User-FTP MUST be able to handle multi-line replies. If the implementation imposes a limit on the number of lines and if this limit is exceeded, the User-FTP MUST recover, e.g., by ignoring the excess lines until the end of the multi-line reply is reached.

A User-FTP SHOULD NOT interpret a 421 reply code ("Service not available, closing control connection") specially, but SHOULD detect closing of the control connection by the server.

DISCUSSION:

  Server implementations that fail to strictly follow the reply rules often cause FTP user programs to hang. Note that RFC-959 resolved ambiguities in the reply rules found in earlier FTP specifications and must be followed.

  It is important to choose FTP reply codes that properly distinguish between temporary and permanent failures, to allow the successful use of file transfer client daemons. These programs depend on the reply codes to decide whether or not to retry a failed transfer; using a permanent failure code (5xx) for a temporary error will cause these programs to give up unnecessarily. When the meaning of a reply matches exactly the text shown in RFC-959, uniformity will be enhanced by using the RFC-959 text verbatim. However, a Server-FTP implementor is encouraged to choose reply text that conveys specific system-dependent information, when appropriate.

Next: 4.1.2.12 Connections: RFC-959 Section 5.2

Connected: An Internet Encyclopedia
RFC 1123 - 4.1.2.11 FTP Replies: RFC-959 Section 4.2, Page 35