Connected: An Internet Encyclopedia
RFC 1122 - 3.2.2.8 Timestamp and Timestamp Reply: RFC-792

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1122
Up: 3. INTERNET LAYER PROTOCOLS
Up: 3.2 PROTOCOL WALK-THROUGH
Up: 3.2.2 Internet Control Message Protocol -- ICMP
Prev: 3.2.2.7 Information Request/Reply: RFC-792
Next: 3.2.2.9 Address Mask Request/Reply: RFC-950

### 3.2.2.8 Timestamp and Timestamp Reply: RFC-792

A host MAY implement Timestamp and Timestamp Reply. If they are implemented, the following rules MUST be followed.

- The ICMP Timestamp server function returns a Timestamp Reply to every Timestamp message that is received. If this function is implemented, it SHOULD be designed for minimum variability in delay (e.g., implemented in the kernel to avoid delay in scheduling a user process).

The following cases for Timestamp are to be handled according to the corresponding rules for ICMP Echo:

- An ICMP Timestamp Request message to an IP broadcast or IP multicast address MAY be silently discarded.

- The IP source address in an ICMP Timestamp Reply MUST be the same as the specific-destination address of the corresponding Timestamp Request message.

- If a Source-route option is received in an ICMP Echo Request, the return route MUST be reversed and used as a Source Route option for the Timestamp Reply message.

- If a Record Route and/or Timestamp option is received in a Timestamp Request, this (these) option(s) SHOULD be updated to include the current host and included in the IP header of the Timestamp Reply message.

- Incoming Timestamp Reply messages MUST be passed up to the ICMP user interface.

The preferred form for a timestamp value (the "standard value") is in units of milliseconds since midnight Universal Time. However, it may be difficult to provide this value with millisecond resolution. For example, many systems use clocks that update only at line frequency, 50 or 60 times per second. Therefore, some latitude is allowed in a "standard value":

1. A "standard value" MUST be updated at least 15 times per second (i.e., at most the six low-order bits of the value may be undefined).

2. The accuracy of a "standard value" MUST approximate that of operator-set CPU clocks, i.e., correct within a few minutes.

Next: 3.2.2.9 Address Mask Request/Reply: RFC-950

Connected: An Internet Encyclopedia
RFC 1122 - 3.2.2.8 Timestamp and Timestamp Reply: RFC-792